(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 134.95 93.5)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/ISENSE_ADC")
	(net 2 "/SCL")
	(net 3 "unconnected-(A1-GPIO5-Pad7)")
	(net 4 "GND")
	(net 5 "unconnected-(A1-VBUS-Pad40)")
	(net 6 "Net-(A1-VSYS)")
	(net 7 "unconnected-(A1-GPIO8-Pad11)")
	(net 8 "/NTC_ADC")
	(net 9 "unconnected-(A1-GPIO15-Pad20)")
	(net 10 "/SD_MOSI")
	(net 11 "/VBAT_ADC")
	(net 12 "/SPI1_MISO")
	(net 13 "/UART0_RX")
	(net 14 "+3.3V")
	(net 15 "/SD_CLK")
	(net 16 "unconnected-(A1-GPIO6-Pad9)")
	(net 17 "/LC_SCK")
	(net 18 "unconnected-(A1-GPIO9-Pad12)")
	(net 19 "/UART0_TX")
	(net 20 "unconnected-(A1-GPIO7-Pad10)")
	(net 21 "/RPM")
	(net 22 "/SPI1_SCK")
	(net 23 "/SD_MISO")
	(net 24 "unconnected-(A1-GPIO14-Pad19)")
	(net 25 "unconnected-(A1-3V3_EN-Pad37)")
	(net 26 "/SDA")
	(net 27 "Net-(A1-ADC_VREF)")
	(net 28 "unconnected-(A1-RUN-Pad30)")
	(net 29 "/SD_CS")
	(net 30 "/SPI1_MOSI")
	(net 31 "unconnected-(A1-GPIO22-Pad29)")
	(net 32 "/SPI1_CSN")
	(net 33 "/LC_DT")
	(net 34 "/DET_B")
	(net 35 "+5V")
	(net 36 "+12V")
	(net 37 "Net-(J10-SHIELD)")
	(net 38 "/DET_A")
	(net 39 "Net-(J10-VDD)")
	(net 40 "Net-(J10-DAT1)")
	(net 41 "Net-(J10-DAT2)")
	(net 42 "Net-(R4-Pad1)")
	(net 43 "Net-(U2-QOD)")
	(net 44 "unconnected-(U2-CT-Pad4)")
	(net 45 "/BOUT_P")
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380"
		(layer "F.Cu")
		(uuid "08ed296e-4ae4-4372-977b-9771afe9350f")
		(at 157.435996 115.985996)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2 ISO7380")
		(property "Reference" "H3"
			(at 0 -2.7 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5f6ab900-ccc7-4716-a10d-c2062d49af86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole"
			(at 0 2.7 0)
			(layer "F.Fab")
			(uuid "c2b5a44a-4391-430a-85f3-d05139ba4f8c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "31f61ef5-a941-44a4-ae26-70052bfd5d11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "96f684d8-beab-45c3-8129-d2e485531685")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*")
		(path "/a993a909-2a59-4bf1-989f-eee5111ee271")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "20b3762f-17a7-49f1-8217-1dc8ebb08191")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c3cd3ed5-8653-4550-8b09-b0b2a53cd7d4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eb91923e-8365-476c-b52b-72f8b94bc283")
			(effects
				(font
					(size 0.88 0.88)
					(thickness 0.13)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(uuid "15c5e754-089f-4bd1-829f-84e7a059e6b5")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(uuid "09f6dd73-335b-4f45-8be2-61548fec3470")
		(at 77.05 104.299999)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -2.63 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "84790df9-1cd5-49ca-b9e4-b03e39a6b498")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "6m"
			(at 0 2.63 0)
			(layer "F.Fab")
			(uuid "ad0b00f5-b751-489a-8aa6-6bce2e4245b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7285933-e52e-490c-be66-7e3a5aee08cf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "82a1786f-7e68-4d56-a9bd-17de798223c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d24cd413-17c6-4d81-9671-9a7e0291eaa2")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.177064 -1.709999)
			(end 2.177063 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "957f8bda-36f0-4650-9663-b2a22ddd96ba")
		)
		(fp_line
			(start -2.177063 1.71)
			(end 2.177064 1.709999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29cac7c3-25b9-423c-9827-6f124d32e6ac")
		)
		(fp_poly
			(pts
				(xy -4 -1.93) (xy -3.999999 1.930001) (xy 4 1.93) (xy 3.999999 -1.930001)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "72be0984-b814-4a0c-9c39-e731506e59ff")
		)
		(fp_poly
			(pts
				(xy -3.15 -1.6) (xy -3.15 1.6) (xy 3.15 1.6) (xy 3.15 -1.6)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "0afaef16-2961-4508-8a71-3ccfb5155169")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b0e72238-0729-458e-991b-d916d0d42192")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.049999 0.000001)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 45 "/BOUT_P")
			(pintype "passive")
			(uuid "b1ff74e7-5afa-484f-8371-55bb1cf242a8")
		)
		(pad "2" smd roundrect
			(at 3.049999 -0.000001)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 36 "+12V")
			(pintype "passive")
			(uuid "5909a937-9840-4607-bd3a-a7a40cf04879")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0ed4f1e0-2d45-4480-80cd-31317bac8636")
		(at 335.184999 16.425 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1b615c50-6d66-4e10-94b6-578e62547eb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5bd5fe1c-03a2-4a7b-b0ec-3d52e55ec857")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "02c7357a-f112-423d-ac24-c4d00129b2ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "76bd56be-0b60-4341-9dfe-8fdaf164eba5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d211e72e-46e8-497b-a8b7-479dadfa3bba")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e83c710-fdd1-4316-add0-0861bce8b9b3")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db5d48a6-6562-42d5-bfa1-8a00c473e8f4")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "fc3758eb-d716-4111-bf8e-a236162d238a")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "549d60e9-8c38-4e49-a22f-55fe52b0b712")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "73a8bb61-b7e0-4014-bf00-34af21382e6d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Net-(J10-SHIELD)")
			(pintype "passive")
			(uuid "c2d7d0bf-a317-4c4f-9598-cb82e16ea9bd")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b56053e9-f899-4d02-b56f-11c346da3058")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "1eeca3f4-76b5-4cb6-be80-5a1fb149811c")
		(at 77.05 110.8 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "250c55f1-a681-4be0-b096-56250e91969f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "92bc14c0-88c5-46c4-aeed-96f568293ed6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "abdd3fb6-f8bb-4010-8729-059dd59e01f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffb90d11-240a-4829-9153-4e8afd953f84")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c3d4036a-7bef-461f-8c0f-d6575eeccf60")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227065 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c86c8c6c-6594-43b1-95b9-e02251b7f75b")
		)
		(fp_line
			(start -0.227065 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b928ca9-aaea-449a-9597-00ede25d378e")
		)
		(fp_poly
			(pts
				(xy -1.85 -0.95) (xy -1.85 0.95) (xy 1.85 0.95) (xy 1.85 -0.95)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "9d68db2b-b8e5-4a6a-9b6e-686eb707f368")
		)
		(fp_poly
			(pts
				(xy -1 -0.625) (xy -1 0.625) (xy 1 0.625) (xy 1 -0.625)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f9a55c61-e015-466b-9852-59071ac42dcb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "919de12f-cfc6-4aba-9add-072db6cd8be6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.000001 -0.000001 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 42 "Net-(R4-Pad1)")
			(pintype "passive")
			(uuid "630abecb-e8b3-4cfc-a58a-3ade928c35e6")
		)
		(pad "2" smd roundrect
			(at 1.000001 0.000001 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "/ISENSE_ADC")
			(pintype "passive")
			(uuid "2b669d02-6d49-4366-875b-2008019bfa3a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "2e0a18ca-d417-4e6e-9094-866b86162564")
		(at 319.25 -7.1 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7a50fd90-06f2-4e6e-bc2f-65437f49ea7d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5c63da80-0dcf-4f39-ac67-12d1d76954f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf9ac49c-3592-43b5-bc28-d515ea38c08a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "94229a48-aac1-4384-bc43-bbf078582b36")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5b34f3fc-8bb6-4638-a780-940b112120a8")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc4db6bd-ba59-410a-96a5-c377daa3dea9")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbce2284-48ec-4302-a430-a51581ed5f10")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "aa5f6c75-752f-451f-ab49-ede779b8adbe")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ee08d6f3-f250-4c3b-86f4-5a77d29045ed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b17d4fdf-2b4c-4221-8398-e6e17cc64334")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(J10-VDD)")
			(pintype "passive")
			(uuid "668573f9-9ec7-4b3e-8e58-2121a756609c")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 41 "Net-(J10-DAT2)")
			(pintype "passive")
			(uuid "045198e7-e8a8-4de7-86ca-7ada3ea77af3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder"
		(layer "F.Cu")
		(uuid "3451c20d-dc71-4b81-9f3d-3aa1274d2304")
		(at 255.47 57.8 180)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "FB1"
			(at 0 -1.55 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "45dd68f4-32c3-4a74-b806-e0d68b9e0487")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FerriteBead_Small"
			(at 0 1.55 180)
			(layer "F.Fab")
			(uuid "6c02407e-3bb9-473c-8465-c2e728150bda")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "332ff167-94de-44a4-9f27-35443aaa2c43")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff76df68-d0f4-43a9-bca6-c0c9d29dbae6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(path "/713d14fd-2012-4816-9456-5b41435cc239")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.410242 0.56)
			(end 0.410242 0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf489c22-05ca-4546-b008-c015a1f11e72")
		)
		(fp_line
			(start -0.410242 -0.56)
			(end 0.410242 -0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13489e66-411f-4212-ac14-de240b1e5f10")
		)
		(fp_rect
			(start -1.93 -0.85)
			(end 1.93 0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a6b1e7f1-80ae-4da1-9955-f512a1fc6ff2")
		)
		(fp_rect
			(start -1 -0.45)
			(end 1 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "411eb6a6-306a-46ed-890f-9b000cb31b3a")
		)
		(pad "1" smd roundrect
			(at -1.15 0 180)
			(size 1.05 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 27 "Net-(A1-ADC_VREF)")
			(pintype "passive")
			(uuid "77b00515-9d2e-45eb-8bf1-e1dcc99cca04")
		)
		(pad "2" smd roundrect
			(at 1.15 0 180)
			(size 1.05 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "9acee768-bff3-4707-881d-19fabad7245b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(uuid "350a5766-3c37-4d31-8908-40b1cb63ebbb")
		(at 64.75 58.5)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J1"
			(at 1 -2.9 0)
			(layer "F.SilkS")
			(uuid "61523c74-7d61-4c59-bfd2-3905d538c92a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "12V_OUT"
			(at 1 4 0)
			(layer "F.Fab")
			(uuid "b6f3393f-b1fc-4cb2-8b65-97108a220e94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "afd4257b-dd28-4e91-985d-b9f519df4867")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "58eb1eb0-1d17-4f54-9371-971cdb824422")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/8f1a8b96-40e7-44f8-a5c1-86f4026568dc")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.36 -2.11)
			(end -2.36 -0.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7ee0ea3-6b26-48d4-87e6-4cd308ce8329")
		)
		(fp_line
			(start -2.06 -0.5)
			(end -1.45 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48478929-79c4-4552-a813-67c698134971")
		)
		(fp_line
			(start -2.06 0.8)
			(end -1.45 0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5c9236e-16d2-4c6b-9ce3-19999f642b20")
		)
		(fp_line
			(start -1.45 -1.2)
			(end -1.45 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cd7e298-9506-41e3-a9b5-bf2c2811cf02")
		)
		(fp_line
			(start -1.45 2.3)
			(end 3.45 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b7bae5d-c025-4721-b61a-24c6947b2592")
		)
		(fp_line
			(start -1.11 -2.11)
			(end -2.36 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2732b646-6b9f-4e61-8454-9834e4818e48")
		)
		(fp_line
			(start -0.6 -2.01)
			(end -0.6 -1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34342138-675d-47d8-a2e0-5fa18ca04ef7")
		)
		(fp_line
			(start -0.3 -2.01)
			(end -0.6 -2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73afe9ff-bdad-4424-bd7b-ea62051d561e")
		)
		(fp_line
			(start -0.3 -1.91)
			(end -0.6 -1.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93db0bb3-4218-4e0d-8cc0-001b3ca2627d")
		)
		(fp_line
			(start -0.3 -1.81)
			(end -0.3 -2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0056ca5b-35ec-4ed8-9ad0-27a8ee61704e")
		)
		(fp_line
			(start 0.5 -1.81)
			(end 0.5 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10732bfd-8cb9-4ec5-8962-29b639aa0f38")
		)
		(fp_line
			(start 0.5 -1.2)
			(end -1.45 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c41445a-631e-4479-85be-1057e83e5271")
		)
		(fp_line
			(start 0.9 1.8)
			(end 1.1 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f20b13d-9149-4b3e-bd5b-75944ff41a86")
		)
		(fp_line
			(start 0.9 2.3)
			(end 0.9 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ddc3c3d-ccec-417b-9958-caf7c9c931ba")
		)
		(fp_line
			(start 1 2.3)
			(end 1 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f409d967-4156-45f5-a802-4b4930419779")
		)
		(fp_line
			(start 1.1 1.8)
			(end 1.1 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11c7039f-54e6-48d1-9ec2-ccbbc3dab29b")
		)
		(fp_line
			(start 1.5 -1.2)
			(end 1.5 -1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa27678b-97ef-4127-9b68-a04595ab183c")
		)
		(fp_line
			(start 3.45 -1.2)
			(end 1.5 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e03013b-9677-45f0-8446-8d96ab10db02")
		)
		(fp_line
			(start 3.45 2.3)
			(end 3.45 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e648b27b-2f8d-40d7-9dd2-bcf7ff05b6de")
		)
		(fp_line
			(start 4.06 -0.5)
			(end 3.45 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59bc5eb8-4473-422e-acca-329678286ae5")
		)
		(fp_line
			(start 4.06 0.8)
			(end 3.45 0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b838485-f6c5-45fe-a02b-95da2b36296d")
		)
		(fp_rect
			(start -2.06 -1.81)
			(end 4.06 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "bf37c230-97cc-470c-a629-7458609e4b7b")
		)
		(fp_rect
			(start -2.45 -2.2)
			(end 4.45 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "181bbcd2-6935-411d-ba94-9ab2e12e8b27")
		)
		(fp_line
			(start -2.36 -2.11)
			(end -2.36 -0.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d85c7df-1085-41e7-9e8c-48a86c1075f8")
		)
		(fp_line
			(start -1.11 -2.11)
			(end -2.36 -2.11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d3ab6ef-f4ee-458e-80bc-ac557eeb58f1")
		)
		(fp_rect
			(start -1.95 -1.7)
			(end 3.95 2.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8333d618-9f4c-4d37-b420-e529ffa9ecac")
		)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
			(uuid "a742c016-c67a-483b-aa00-8135ffee9dd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 36 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0bbad621-2a60-4917-b14e-3239fe3dd76f")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "eb2c571b-f8e4-475b-8bc0-38862c625bf9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380"
		(layer "F.Cu")
		(uuid "4228679b-7286-4477-9b46-525f7c8bef75")
		(at 112.464004 115.985996)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2 ISO7380")
		(property "Reference" "H4"
			(at 0 -2.7 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "45e821ab-c77c-4bd7-a3ea-0509f25b7f6f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole"
			(at 0 2.7 0)
			(layer "F.Fab")
			(uuid "3d1ddc34-ef44-4ef2-81e8-a6da1203cc0b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e04bb6ee-ce32-4b0a-b210-5ff5d2e0f950")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "425f9451-a295-4779-8225-ab927b362fe4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*")
		(path "/687fab0b-04e8-490a-ab5b-e420b0bf5ce0")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "53206763-f391-4b04-9098-a88584f2a903")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "e6ce90bb-e124-4910-a0fc-0c9aeb870a9d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8940e8fa-5bbf-486c-bb3e-c76947127250")
			(effects
				(font
					(size 0.88 0.88)
					(thickness 0.13)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(uuid "05ac9591-d76f-441a-93e5-11592659de20")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "47ba0019-57d3-4f08-86cd-49ccff7cc2ab")
		(at 80.15 108.4 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "54dbc31f-823b-4f42-b19c-24a37cc34981")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "8848c62e-cc3b-410e-bd13-f44f74ec5a2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "16ef63be-53ec-438e-b987-ebf76c16cf2f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5948b50-fa51-4913-8d28-b913b52d0152")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/300b61c4-49f1-47fe-85db-48811216a59b")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227065 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19dd28f4-db25-48c5-a009-ca3afe4b5e87")
		)
		(fp_line
			(start -0.227065 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "afb64317-b005-4aee-8dfd-387d41a383bd")
		)
		(fp_poly
			(pts
				(xy -1.85 -0.95) (xy 1.85 -0.95) (xy 1.85 0.95) (xy -1.85 0.95)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "bb7512ac-0729-4c61-9ab8-b1f2b4c47ef2")
		)
		(fp_poly
			(pts
				(xy -1 -0.625) (xy 1 -0.625) (xy 1 0.625) (xy -1 0.625)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "387cf24c-f596-4c17-95f5-2a8f600c6f5a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6664d3c2-61d3-4b04-8a03-37781c87c8dd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.000001 -0.000001 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 36 "+12V")
			(pintype "passive")
			(uuid "00bce192-2d2c-4dac-bfbe-0134d9a06f6c")
		)
		(pad "2" smd roundrect
			(at 1.000001 0.000001 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "/VBAT_ADC")
			(pintype "passive")
			(uuid "387db30b-a044-49ea-8882-6eb9417c74dd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMB"
		(layer "F.Cu")
		(uuid "61df66f5-877d-4e8f-a384-71722cf77504")
		(at 235.8 23.1)
		(descr "Diode SMB (DO-214AA)")
		(tags "Diode SMB (DO-214AA)")
		(property "Reference" "D1"
			(at 0 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c49f9a00-7103-49ad-b476-bdda601a7ca2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "B220"
			(at 0 3.1 0)
			(layer "F.Fab")
			(uuid "103c0a33-3711-405a-be8e-cbe3ba0facce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b4c72f9-8539-4e3e-b79c-bc639a778f38")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "20V 2A Schottky Barrier Rectifier Diode, SMB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a0a4cc5-809f-46a6-aad0-001ff13e0515")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "D*SMB*")
		(path "/f417715e-a175-4a8c-a505-861be29242c9")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.66 -2.15)
			(end -3.66 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3aa09dce-9361-4def-b557-d7f46c205ff5")
		)
		(fp_line
			(start -3.66 -2.15)
			(end 2.15 -2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf5a9e74-5605-440d-b1fc-568c165986b4")
		)
		(fp_line
			(start -3.66 2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbe4c492-2896-4901-a289-c91c6bc930eb")
		)
		(fp_line
			(start -3.65 -2.25)
			(end 3.65 -2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e92d3bc-ff10-461e-b7a7-581cd6580d3f")
		)
		(fp_line
			(start -3.65 2.25)
			(end -3.65 -2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61e5772a-43ed-49d2-ab94-ac75e146f9ed")
		)
		(fp_line
			(start 3.65 -2.25)
			(end 3.65 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1495ee2e-a20e-4c1a-852c-6bb8a5ae9539")
		)
		(fp_line
			(start 3.65 2.25)
			(end -3.65 2.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8dde31e2-3209-46f0-909d-64b95a22d14a")
		)
		(fp_line
			(start -2.3 2)
			(end -2.3 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a5f41c23-9b2a-4e65-81c1-d1114f85c2e4")
		)
		(fp_line
			(start -0.64944 -0.79908)
			(end -0.64944 0.80112)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de117256-c7a1-47db-a24e-eaf9adc1e87e")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end -1.55114 0.00102)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe7d5700-080d-4301-8ff1-b9075f8ff573")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end 0.50118 -0.79908)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3372ae1a-78c5-457a-9d3f-b0833f8fdd86")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end 0.50118 0.75032)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "474af094-c923-476a-b81a-007d0e2e5e14")
		)
		(fp_line
			(start 0.50118 0.00102)
			(end 1.4994 0.00102)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea1eb47a-6ad5-4559-856f-01e88b6fe45a")
		)
		(fp_line
			(start 0.50118 0.75032)
			(end 0.50118 -0.79908)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df8f0943-5031-403c-8ffe-795dcc6b1c02")
		)
		(fp_line
			(start 2.3 -2)
			(end -2.3 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d13ef68d-8dfb-41df-b305-2141aa751e04")
		)
		(fp_line
			(start 2.3 -2)
			(end 2.3 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7417fde-427d-43a9-9008-66affef81fd0")
		)
		(fp_line
			(start 2.3 2)
			(end -2.3 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70ed4b5e-1a35-4ac4-93fa-0fade496d5a9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3 0)
			(layer "F.Fab")
			(uuid "12155f8b-08bf-496d-b1f1-8ac68572054b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.15 0)
			(size 2.5 2.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1086956522)
			(net 6 "Net-(A1-VSYS)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "29033335-2d35-4e2b-8290-3d20cf591608")
		)
		(pad "2" smd roundrect
			(at 2.15 0)
			(size 2.5 2.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1086956522)
			(net 35 "+5V")
			(pinfunction "A")
			(pintype "passive")
			(uuid "c5300234-2bfd-47e5-b967-4ca316c9c372")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "65fa1262-5374-4959-89bf-81e81c77f487")
		(at 317.934999 8.425 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8088a28d-670a-4bd4-8149-17c30dbbdb2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "89e92683-83f9-41a6-bc26-7c6e6594b110")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "985cf52d-ad1c-48be-880d-fe009fde84bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "81ec0d5e-8534-4a9f-900d-27641db3fd46")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e890d78c-7d88-4815-8144-56cbb98ab004")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27c2f9de-878f-4ce4-8cb4-8111f2c8f1fc")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d16ecda-df4e-4b00-a621-a2fd8f222b3a")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "6de68739-2061-4972-b803-20db0019e959")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8205814f-59f4-4d7c-a6f1-d7ad44904c32")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fc134004-a0e8-425f-8aee-563dc3e71a48")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 34 "/DET_B")
			(pintype "passive")
			(uuid "e365cc44-cd55-4301-a45d-2d897a5931fd")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "GND")
			(pintype "passive")
			(uuid "d669070b-fc97-4a0a-9a3e-b95095bb958b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "689edfed-879f-4fb2-b839-388fcf067cd6")
		(at 252.45 27.9929)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "586fb4cf-9ff1-46f6-a4b2-93774c7d4fe4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a9f08806-0042-4b90-bdec-915c9e044081")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c7cc436-e6fb-4de9-be84-ff779131e548")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fc5e6bc-793e-4c89-bc3c-ae9459f414fd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a63e4373-1167-490f-8c68-4898c20e903d")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59b3722f-aaf0-4a9c-8636-3313a6d8892b")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71abcd7c-8a02-47a0-bb5f-392ecf297e60")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a3e096ac-1873-4dec-819b-3a04778c3f8c")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1c30ad12-6f6a-44bd-b60c-360653412254")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "44045076-f4a2-443a-bc53-921188da8921")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "d7187348-800f-4bae-bff6-136cd63e1e1e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 26 "/SDA")
			(pintype "passive")
			(uuid "734dbde1-c3c3-48bc-8f21-f7ade7bcc6f5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:RaspberryPi_Pico_Common_THT"
		(layer "F.Cu")
		(uuid "6b026c79-6d44-410a-bf56-4fd17b396bf0")
		(at 137.77 69.16)
		(descr "Raspberry Pi Pico common (Pico & Pico W) through-hole footprint, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb antenna")
		(property "Reference" "A1"
			(at 20.6375 48.895 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1f86eb29-eaa7-4f84-9caf-4c5e0fd7a75e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify left)
			)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 8.89 52.07 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "79def01a-9fdf-460a-af9e-748d3bfd7b6c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 8.89 24.13 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "86f46e72-c723-407f-bf56-67003e24196f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN; also supports Raspberry Pi Pico 2 W"
			(at 8.89 24.13 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0409a48b-e6dd-443a-af82-fbf2bcf7d3ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RaspberryPi?Pico?Common* RaspberryPi?Pico?W?SMD*")
		(path "/11bc55dd-0742-4949-be37-dfcac6ae03ff")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.04 0.8)
			(end -2.04 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "670ca6ab-e8d8-42b3-bc75-cf427edeb08b")
		)
		(fp_line
			(start -1.72 -0.87)
			(end -1.72 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11964d5d-91c8-424b-a0ed-649cb677829d")
		)
		(fp_line
			(start -1.38 -1.417)
			(end -1.38 49.677)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27dccfd5-cee3-461a-bed0-b6c6dae28cef")
		)
		(fp_line
			(start -1.11 -1.48)
			(end 1.38 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63a2d4f9-bead-40e2-a689-07d777ff3ae7")
		)
		(fp_line
			(start -1.11 49.74)
			(end 2.727939 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55e546c9-aadb-4537-aefe-e13f38daf455")
		)
		(fp_line
			(start 1.38 -1.48)
			(end 1.38 -0.56648)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b9fb0af-2676-4387-acb3-2eed5feca2d2")
		)
		(fp_line
			(start 1.38 -1.48)
			(end 2.72794 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f068d8c-25d8-4ce3-9131-e5590d4c5101")
		)
		(fp_line
			(start 1.38 1.82648)
			(end 1.38 46.43352)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d456970-367a-4d50-b7ec-aafcd5d35a55")
		)
		(fp_line
			(start 1.38 48.82648)
			(end 1.38 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f40bc013-8887-4a92-9b0e-c346582ecc8e")
		)
		(fp_line
			(start 3.652061 -1.48)
			(end 4.655 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9bdfa5e-3c95-4dd4-989e-7ec83131d4ee")
		)
		(fp_line
			(start 4.655 -1.48)
			(end 13.125 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23c02d56-d1af-433d-a1bc-fa0eff51697e")
		)
		(fp_line
			(start 4.78 -2.78)
			(end 4.78 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36949b7f-0e18-4dc4-8738-88856ff174fe")
		)
		(fp_line
			(start 4.78 -2.78)
			(end 13 -2.78)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59dafbd9-c79c-4913-8a9a-16fe9a7e2608")
		)
		(fp_line
			(start 4.78 -1.96)
			(end 4.99 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "819ec14b-3852-4fbb-a683-8355c88b714e")
		)
		(fp_line
			(start 4.99 -1.96)
			(end 4.99 -0.564)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87853980-8212-4347-9217-543c3d9a77bc")
		)
		(fp_line
			(start 4.99 1.824)
			(end 4.99 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37fbd596-7edc-4999-822a-afacd1aa9131")
		)
		(fp_line
			(start 5.29 49.74)
			(end 3.652061 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65ac225d-67bd-44f3-bf7f-f6627d8dadad")
		)
		(fp_line
			(start 12.49 49.74)
			(end 5.29 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd24a2c7-55dc-4f53-8597-36cd957f6f81")
		)
		(fp_line
			(start 12.79 -1.96)
			(end 12.79 -0.564)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f96f9fb-206e-4b09-8993-9efa9a4d7ace")
		)
		(fp_line
			(start 12.79 1.824)
			(end 12.79 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04b9c06e-041a-4aaf-9ce9-aaf2482163fd")
		)
		(fp_line
			(start 12.79 3.04)
			(end 4.99 3.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1fcecc7-f546-449a-93c7-2fd87bb8b6c7")
		)
		(fp_line
			(start 13 -2.78)
			(end 13 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e06b4ce7-5d40-4522-b533-ee50cc4c4237")
		)
		(fp_line
			(start 13 -1.96)
			(end 12.79 -1.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff675bb8-a409-4fc1-b256-128d711a6198")
		)
		(fp_line
			(start 13.125 -1.48)
			(end 14.127939 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65dc489a-4938-429c-93fd-7e622d75f89e")
		)
		(fp_line
			(start 14.127939 49.74)
			(end 12.49 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30777c6f-9692-4259-bc87-dfbd17223baf")
		)
		(fp_line
			(start 15.052061 -1.48)
			(end 16.4 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e52df8f3-c826-499a-ac9c-1596a3cb071c")
		)
		(fp_line
			(start 15.052061 49.74)
			(end 18.89 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac3f3727-59c1-4692-9af2-efb16e2f7e1b")
		)
		(fp_line
			(start 16.4 -1.48)
			(end 16.4 -0.56648)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de1d1bc7-ef23-4bc8-b8ff-430de578d03d")
		)
		(fp_line
			(start 16.4 1.82648)
			(end 16.4 46.43352)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "451db6e6-2cfb-4c7f-966f-1c1701f13a39")
		)
		(fp_line
			(start 16.4 48.82648)
			(end 16.4 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25769b5f-b2af-4d4a-b636-48359bb838eb")
		)
		(fp_line
			(start 18.89 -1.48)
			(end 16.4 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0afb4810-ae17-4572-83fd-7bc71d2aecab")
		)
		(fp_line
			(start 19.16 49.677)
			(end 19.16 -1.417)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aff70922-5108-4c69-b069-eec43a0ad867")
		)
		(fp_line
			(start 19.5 -0.87)
			(end 19.5 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78f020e9-5656-4939-a961-b59e87cfbedc")
		)
		(fp_arc
			(start -1.72 -0.87)
			(mid -1.541335 -1.301335)
			(end -1.11 -1.48)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46e4f71d-a0ae-4263-b784-4588b0110983")
		)
		(fp_arc
			(start -1.11 49.74)
			(mid -1.541364 49.561364)
			(end -1.72 49.13)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e5478bb-c086-482c-943b-5ad27b47b7ca")
		)
		(fp_arc
			(start 18.89 -1.48)
			(mid 19.321335 -1.301335)
			(end 19.5 -0.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e4b988a-2f84-41cb-979c-b64b46c8d455")
		)
		(fp_arc
			(start 19.5 49.13)
			(mid 19.321335 49.561335)
			(end 18.89 49.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edb31dcf-9345-4930-bbf4-59d73e84afa2")
		)
		(fp_circle
			(center 3.19 0.63)
			(end 4.24 0.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "7890184f-83ec-4933-972c-a22ade3a32df")
		)
		(fp_circle
			(center 3.19 47.63)
			(end 4.24 47.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "9942c6e3-6cf6-4e3c-a14b-01fd378c3dbc")
		)
		(fp_circle
			(center 14.59 0.63)
			(end 15.64 0.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "0c05003a-b71e-469f-8101-286889faeb2c")
		)
		(fp_circle
			(center 14.59 47.63)
			(end 15.64 47.63)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "c93ad866-e22f-452d-89e0-72d97b973f80")
		)
		(fp_poly
			(pts
				(xy 4.39 -3.17) (xy 13.39 -3.17) (xy 13.39 -1.62) (xy 20.43 -1.62) (xy 20.43 50.68) (xy -2.65 50.68)
				(xy -2.65 -1.62) (xy 4.39 -1.62)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "210f5bcb-9e69-4d19-971d-3a82241b6424")
		)
		(fp_line
			(start -1.61 -0.37)
			(end -0.61 -1.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61a52b96-90e1-4d8d-a794-d8c584569097")
		)
		(fp_line
			(start -1.61 49.13)
			(end -1.61 -0.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90938875-afaf-4fb3-8d74-236094d3ed2e")
		)
		(fp_line
			(start -0.61 -1.37)
			(end 18.89 -1.37)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9874643e-14a4-4044-95ce-8046501586ae")
		)
		(fp_line
			(start 4.265 10.055)
			(end 4.265 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e6933e7-ed65-4cc1-af88-9a8c3170cecd")
		)
		(fp_line
			(start 6.515 10.055)
			(end 6.515 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33abec31-1dcf-4724-aa7a-71034d0949fa")
		)
		(fp_line
			(start 18.89 49.63)
			(end -1.11 49.63)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56a34af1-1b71-4044-9f6f-86aef14a5823")
		)
		(fp_line
			(start 19.39 -0.87)
			(end 19.39 49.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99ffe233-6cf8-4763-a6c2-38be62e3e710")
		)
		(fp_rect
			(start 2.39 3.03)
			(end 3.99 3.83)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d56794f2-1674-4506-b8f4-b4017c7d0065")
		)
		(fp_rect
			(start 2.69 3.03)
			(end 3.69 3.83)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "9b142f39-0f13-4913-b8d6-1282018a8348")
		)
		(fp_rect
			(start 3.79 8.505)
			(end 6.99 12.755)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f24bb073-aadf-426d-b8f7-05654776a8c5")
		)
		(fp_arc
			(start -1.11 49.63)
			(mid -1.463553 49.483553)
			(end -1.61 49.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "499daddc-fce1-4599-bf45-59bfb8ddb6f6")
		)
		(fp_arc
			(start 4.265 10.055)
			(mid 5.39 8.93)
			(end 6.515 10.055)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffe922bf-f5ed-4179-9d46-0be3ff757766")
		)
		(fp_arc
			(start 6.515 11.205)
			(mid 5.39 12.33)
			(end 4.265 11.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d924c4e-1fc1-4cb4-94e4-db6e4372a994")
		)
		(fp_arc
			(start 18.89 -1.37)
			(mid 19.243553 -1.223553)
			(end 19.39 -0.87)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07c94b1c-5ca1-463d-bb29-a8c16a1e1108")
		)
		(fp_arc
			(start 19.39 49.13)
			(mid 19.243553 49.483553)
			(end 18.89 49.63)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0f24534-0c06-41bf-b884-f3e2af9ed1b9")
		)
		(fp_poly
			(pts
				(xy 12.68 2.93) (xy 12.68 -2.07) (xy 12.89 -2.07) (xy 12.89 -2.67) (xy 4.89 -2.67) (xy 4.89 -2.07)
				(xy 5.1 -2.07) (xy 5.1 2.93)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d1619221-e1a1-4c7f-98de-5475965c779f")
		)
		(fp_text user "USB Cable"
			(at 8.89 -13.335 0)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "27faad95-019a-45c1-a838-1f394f4ca083")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "Possible Antenna"
			(at 8.89 43.815 0)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "44270769-b27d-4dcb-9191-f9e4c53e1d6a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "Keep Out"
			(at 8.89 45.72 0)
			(unlocked yes)
			(layer "Cmts.User")
			(uuid "d8496fdd-8d40-47d0-a88a-339bfbb34298")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 8.89 24.13 90)
			(layer "F.Fab")
			(uuid "615cc516-a126-4613-a9d0-3c7f924b9a91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 26 "/SDA")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
			(uuid "d5448d0c-268e-4928-846d-2ed0d095e38d")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SCL")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
			(uuid "0b93e29b-a871-4387-917e-9a4e4c3188f2")
		)
		(pad "3" thru_hole custom
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "a721b7ef-6129-4b4f-bb4d-a8e148e83819")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/RPM")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
			(uuid "799b5676-3dea-4629-b164-06d1b586012d")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/LC_DT")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
			(uuid "ffd5b5d6-7a5f-4ebd-9b79-7cb30995edba")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/LC_SCK")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
			(uuid "75cec292-e4e4-4342-b66c-b75dbb698864")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional+no_connect")
			(uuid "0d18261a-34ee-4d48-8f14-406a7c3355ce")
		)
		(pad "8" thru_hole custom
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "a180c381-d1f8-4680-a527-5729db63e435")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional+no_connect")
			(uuid "7062cd9b-82e3-46c9-809f-c7492fe751d4")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional+no_connect")
			(uuid "78ecff5f-f706-4e68-8b12-79d1fbc2c8a9")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(A1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional+no_connect")
			(uuid "3878de1a-e768-424d-9041-e2bb4f970656")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
			(uuid "7600ae81-742b-4be4-b028-41b39fb40b8f")
		)
		(pad "13" thru_hole custom
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "321f94e5-c14e-4e09-a17e-266d9ac8aced")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SPI1_SCK")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
			(uuid "b4538e44-5c09-4f66-acd4-7a655b73cc69")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/SPI1_MOSI")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
			(uuid "e91dd0c7-2c19-4cec-92d5-4b933feac91a")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SPI1_MISO")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
			(uuid "5779c834-cfb0-40be-8186-d5e08be41bd3")
		)
		(pad "17" thru_hole circle
			(at 0 40.64)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/SPI1_CSN")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
			(uuid "f2dc14c4-b1b7-4890-bcf9-66a6e4d0abfc")
		)
		(pad "18" thru_hole custom
			(at 0 43.18)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "beb0ee7c-5efb-4287-babd-8eda72bb3b47")
		)
		(pad "19" thru_hole circle
			(at 0 45.72)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-GPIO14-Pad19)")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
			(uuid "c3f70d02-ad2e-40ce-aa8d-4861780070cf")
		)
		(pad "20" thru_hole circle
			(at 0 48.26)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-GPIO15-Pad20)")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
			(uuid "491eb0a9-512f-432b-aa32-001546b10a3c")
		)
		(pad "21" thru_hole circle
			(at 17.78 48.26)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/UART0_TX")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
			(uuid "76eed332-1cc7-4154-bb0e-f6274d1eb430")
		)
		(pad "22" thru_hole circle
			(at 17.78 45.72)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/UART0_RX")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
			(uuid "5f33db09-5a56-4d9d-ab21-05e52be24d8f")
		)
		(pad "23" thru_hole custom
			(at 17.78 43.18)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "4cbe62a2-1e1a-48c4-a791-f5c531319016")
		)
		(pad "24" thru_hole circle
			(at 17.78 40.64)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/SD_CLK")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
			(uuid "6be378f7-6ef0-4cbe-a4f0-be6a7e455b5b")
		)
		(pad "25" thru_hole circle
			(at 17.78 38.1)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/SD_MOSI")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
			(uuid "4a1d4ba3-cb4b-4045-a6e9-28e806645306")
		)
		(pad "26" thru_hole circle
			(at 17.78 35.56)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SD_MISO")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(uuid "c29613bc-1044-4643-b03a-2322f96738f7")
		)
		(pad "27" thru_hole circle
			(at 17.78 33.02)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/SD_CS")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(uuid "e8e61842-21ed-4dd4-b0df-b6266c679191")
		)
		(pad "28" thru_hole custom
			(at 17.78 30.48)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "10667352-8090-4ad2-9721-461edfe9bb72")
		)
		(pad "29" thru_hole circle
			(at 17.78 27.94)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(A1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
			(uuid "ebfbfab5-7795-4ac5-a0f4-5fc617fc07c7")
		)
		(pad "30" thru_hole circle
			(at 17.78 25.4)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "passive+no_connect")
			(uuid "e61a6990-5c96-4027-9d7c-7691a169c10f")
		)
		(pad "31" thru_hole circle
			(at 17.78 22.86)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/VBAT_ADC")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
			(uuid "546f433b-8f60-45c5-99d5-6f46f61cb3a4")
		)
		(pad "32" thru_hole circle
			(at 17.78 20.32)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/ISENSE_ADC")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
			(uuid "047dfd76-ab46-41ba-8cca-04eabf4cef5a")
		)
		(pad "33" thru_hole custom
			(at 17.78 17.78)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "AGND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "284d0554-32e8-4c71-b0ed-8c8ef22ef1ea")
		)
		(pad "34" thru_hole circle
			(at 17.78 15.24)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/NTC_ADC")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
			(uuid "3dcc72e5-41be-4997-a53e-bf11cba441ed")
		)
		(pad "35" thru_hole circle
			(at 17.78 12.7)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(A1-ADC_VREF)")
			(pinfunction "ADC_VREF")
			(pintype "power_in")
			(uuid "dd41c59e-9495-4fac-8fd0-6750ef4a7b29")
		)
		(pad "36" thru_hole circle
			(at 17.78 10.16)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_out")
			(uuid "6a0cd008-072e-4885-80de-d0200ab137d3")
		)
		(pad "37" thru_hole circle
			(at 17.78 7.62)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "passive+no_connect")
			(uuid "c9ba6076-2b21-49d7-931e-4be8ed7b6457")
		)
		(pad "38" thru_hole custom
			(at 17.78 5.08)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
			(uuid "755a53b6-6bb7-497e-9f77-e8b06cc9a5d6")
		)
		(pad "39" thru_hole circle
			(at 17.78 2.54)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(A1-VSYS)")
			(pinfunction "VSYS")
			(pintype "power_in")
			(uuid "3557b90e-a6b8-4e2b-ac36-d79b805c984e")
		)
		(pad "40" thru_hole circle
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_out+no_connect")
			(uuid "204e8ebf-620b-4793-a796-5f0e4d4ca92b")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu" "F.Paste" "B.Paste")
			(uuid "473f8cdf-6a2f-4fca-9ad1-6c9141959025")
			(name "Antenna Copper Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 144.26 118.279895) (xy 139.56 114.629895) (xy 139.56 110.29) (xy 153.76 110.29) (xy 153.76 114.629895)
					(xy 149.06 118.279895) (xy 149.06 119.29) (xy 144.26 119.29)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.CrtYd")
			(uuid "4a9003cf-39fc-4a63-948f-f6660c3602cb")
			(name "USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 140.91 65.59) (xy 142.72 65.59) (xy 142.72 65.99) (xy 150.6 65.99) (xy 150.6 65.59) (xy 152.41 65.59)
					(xy 152.41 46.09) (xy 140.91 46.09)
				)
			)
		)
		(group ""
			(uuid "c57c3bcf-f78c-4fc1-94e0-d71c83611509")
			(members "047dfd76-ab46-41ba-8cca-04eabf4cef5a" "0afb4810-ae17-4572-83fd-7bc71d2aecab"
				"0b93e29b-a871-4387-917e-9a4e4c3188f2" "0d18261a-34ee-4d48-8f14-406a7c3355ce"
				"10667352-8090-4ad2-9721-461edfe9bb72" "204e8ebf-620b-4793-a796-5f0e4d4ca92b"
				"25769b5f-b2af-4d4a-b636-48359bb838eb" "284d0554-32e8-4c71-b0ed-8c8ef22ef1ea"
				"321f94e5-c14e-4e09-a17e-266d9ac8aced" "3557b90e-a6b8-4e2b-ac36-d79b805c984e"
				"3878de1a-e768-424d-9041-e2bb4f970656" "3dcc72e5-41be-4997-a53e-bf11cba441ed"
				"451db6e6-2cfb-4c7f-966f-1c1701f13a39" "491eb0a9-512f-432b-aa32-001546b10a3c"
				"4a1d4ba3-cb4b-4045-a6e9-28e806645306" "4cbe62a2-1e1a-48c4-a791-f5c531319016"
				"4d456970-367a-4d50-b7ec-aafcd5d35a55" "546f433b-8f60-45c5-99d5-6f46f61cb3a4"
				"5779c834-cfb0-40be-8186-d5e08be41bd3" "5b9fb0af-2676-4387-acb3-2eed5feca2d2"
				"5f33db09-5a56-4d9d-ab21-05e52be24d8f" "63a2d4f9-bead-40e2-a689-07d777ff3ae7"
				"6a0cd008-072e-4885-80de-d0200ab137d3" "6be378f7-6ef0-4cbe-a4f0-be6a7e455b5b"
				"7062cd9b-82e3-46c9-809f-c7492fe751d4" "755a53b6-6bb7-497e-9f77-e8b06cc9a5d6"
				"75cec292-e4e4-4342-b66c-b75dbb698864" "7600ae81-742b-4be4-b028-41b39fb40b8f"
				"76eed332-1cc7-4154-bb0e-f6274d1eb430" "78ecff5f-f706-4e68-8b12-79d1fbc2c8a9"
				"799b5676-3dea-4629-b164-06d1b586012d" "a180c381-d1f8-4680-a527-5729db63e435"
				"a721b7ef-6129-4b4f-bb4d-a8e148e83819" "b4538e44-5c09-4f66-acd4-7a655b73cc69"
				"beb0ee7c-5efb-4287-babd-8eda72bb3b47" "c29613bc-1044-4643-b03a-2322f96738f7"
				"c3f70d02-ad2e-40ce-aa8d-4861780070cf" "c9ba6076-2b21-49d7-931e-4be8ed7b6457"
				"d5448d0c-268e-4928-846d-2ed0d095e38d" "dd41c59e-9495-4fac-8fd0-6750ef4a7b29"
				"de1d1bc7-ef23-4bc8-b8ff-430de578d03d" "e61a6990-5c96-4027-9d7c-7691a169c10f"
				"e8e61842-21ed-4dd4-b0df-b6266c679191" "e91dd0c7-2c19-4cec-92d5-4b933feac91a"
				"ebfbfab5-7795-4ac5-a0f4-5fc617fc07c7" "f2dc14c4-b1b7-4890-bcf9-66a6e4d0abfc"
				"f40bc013-8887-4a92-9b0e-c346582ecc8e" "ffd5b5d6-7a5f-4ebd-9b79-7cb30995edba"
			)
		)
		(group ""
			(uuid "6e3485c9-8dab-42cf-95d9-94624e12dcf6")
			(members "44270769-b27d-4dcb-9191-f9e4c53e1d6a" "473f8cdf-6a2f-4fca-9ad1-6c9141959025"
				"4e5478bb-c086-482c-943b-5ad27b47b7ca" "bd24a2c7-55dc-4f53-8597-36cd957f6f81"
				"d8496fdd-8d40-47d0-a88a-339bfbb34298" "edb31dcf-9345-4930-bbf4-59d73e84afa2"
			)
		)
		(group ""
			(uuid "91bf35f5-b8c4-4b49-abef-b2c57dd38578")
			(members "04b9c06e-041a-4aaf-9ce9-aaf2482163fd" "23c02d56-d1af-433d-a1bc-fa0eff51697e"
				"36949b7f-0e18-4dc4-8738-88856ff174fe" "37fbd596-7edc-4999-822a-afacd1aa9131"
				"59dafbd9-c79c-4913-8a9a-16fe9a7e2608" "819ec14b-3852-4fbb-a683-8355c88b714e"
				"87853980-8212-4347-9217-543c3d9a77bc" "9f96f9fb-206e-4b09-8993-9efa9a4d7ace"
				"a1fcecc7-f546-449a-93c7-2fd87bb8b6c7" "e06b4ce7-5d40-4522-b533-ee50cc4c4237"
				"ff675bb8-a409-4fc1-b256-128d711a6198"
			)
		)
		(group ""
			(uuid "a3da2e14-93d1-4557-b3c3-bbea24908526")
			(members "11964d5d-91c8-424b-a0ed-649cb677829d" "27dccfd5-cee3-461a-bed0-b6c6dae28cef"
				"46e4f71d-a0ae-4263-b784-4588b0110983" "5e4b988a-2f84-41cb-979c-b64b46c8d455"
				"670ca6ab-e8d8-42b3-bc75-cf427edeb08b" "78f020e9-5656-4939-a961-b59e87cfbedc"
				"aff70922-5108-4c69-b069-eec43a0ad867"
			)
		)
		(group ""
			(uuid "f6087fa4-9b4c-4356-b62c-66707152cfc5")
			(members "0c05003a-b71e-469f-8101-286889faeb2c" "30777c6f-9692-4259-bc87-dfbd17223baf"
				"3f068d8c-25d8-4ce3-9131-e5590d4c5101" "55e546c9-aadb-4537-aefe-e13f38daf455"
				"65ac225d-67bd-44f3-bf7f-f6627d8dadad" "65dc489a-4938-429c-93fd-7e622d75f89e"
				"7890184f-83ec-4933-972c-a22ade3a32df" "9942c6e3-6cf6-4e3c-a14b-01fd378c3dbc"
				"a9bdfa5e-3c95-4dd4-989e-7ec83131d4ee" "ac3f3727-59c1-4692-9af2-efb16e2f7e1b"
				"c93ad866-e22f-452d-89e0-72d97b973f80" "e52df8f3-c826-499a-ac9c-1596a3cb071c"
			)
		)
		(group ""
			(uuid "77e87dfd-da91-4a2d-bd40-6e58dd75b9c2")
			(members "07c94b1c-5ca1-463d-bb29-a8c16a1e1108" "210f5bcb-9e69-4d19-971d-3a82241b6424"
				"27faad95-019a-45c1-a838-1f394f4ca083" "33abec31-1dcf-4724-aa7a-71034d0949fa"
				"499daddc-fce1-4599-bf45-59bfb8ddb6f6" "4a9003cf-39fc-4a63-948f-f6660c3602cb"
				"56a34af1-1b71-4044-9f6f-86aef14a5823" "5d924c4e-1fc1-4cb4-94e4-db6e4372a994"
				"615cc516-a126-4613-a9d0-3c7f924b9a91" "61a52b96-90e1-4d8d-a794-d8c584569097"
				"7e6933e7-ed65-4cc1-af88-9a8c3170cecd" "90938875-afaf-4fb3-8d74-236094d3ed2e"
				"9874643e-14a4-4044-95ce-8046501586ae" "99ffe233-6cf8-4763-a6c2-38be62e3e710"
				"9b142f39-0f13-4913-b8d6-1282018a8348" "b0f24534-0c06-41bf-b884-f3e2af9ed1b9"
				"d1619221-e1a1-4c7f-98de-5475965c779f" "d56794f2-1674-4506-b8f4-b4017c7d0065"
				"f24bb073-aadf-426d-b8f7-05654776a8c5" "ffe922bf-f5ed-4179-9d46-0be3ff757766"
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_PinSockets_H8.50mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.step"
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6d8b5b4e-47cf-4f3c-8072-7ec0ae6c1cc5")
		(at 73.65 110 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7d6ebb25-eacb-465f-8b21-0fb0c4052865")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "c6be3f82-1486-4f13-bed9-57f1d2fc8649")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "14d4f5ce-5d75-4849-821a-17e937894a9d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7f50baa-5f91-46ae-874c-6028c85dcd6d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3505b6b9-ff0a-43a3-a5ac-a96c312cff17")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "deece9c6-6ae9-4358-a59b-3986577ca69a")
		)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d3c340a-b477-4a3c-85be-70cada36f744")
		)
		(fp_poly
			(pts
				(xy -1.879999 -0.98) (xy 1.88 -0.98) (xy 1.879999 0.98) (xy -1.88 0.98)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "dda2f9c4-f2cd-4e8e-a9a8-0a49b53cd603")
		)
		(fp_poly
			(pts
				(xy -1 -0.625) (xy 1 -0.625) (xy 1 0.625) (xy -1 0.625)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f900df5f-55af-4271-b0f3-feaff00082b6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ac664085-5f36-4f5a-8c39-677a727df369")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "28f98e2e-aadc-406b-857d-73e828c60e61")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "fa507854-ad2e-48c7-af6b-3f0b2ed03ab8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380"
		(layer "F.Cu")
		(uuid "6dcf7358-c2ca-4b6c-aa38-6ef46d2429f1")
		(at 157.435996 71.014004)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2 ISO7380")
		(property "Reference" "H2"
			(at 0 -2.7 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "16beb9c6-8505-4d98-9332-215a20ea4ee4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole"
			(at 0 2.7 0)
			(layer "F.Fab")
			(uuid "77244e73-7647-425b-a3b6-57e410214d2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "879956be-a890-47f8-b1fb-999262fbbd95")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "101cd4d7-fabc-42b8-b261-57bf5d145ea6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*")
		(path "/1593f1ba-4f4a-4ef2-b702-d858c2011873")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "17297fc8-9b30-48e1-8d9c-ec51cdcb79d6")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ed53427e-0c0b-48f1-b0ff-c27bb01e6b88")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a6143238-7a4a-44fe-af6c-dd6211eea93c")
			(effects
				(font
					(size 0.88 0.88)
					(thickness 0.13)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(uuid "73a87bad-946a-434e-ab0e-2c271cf3d7b2")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380"
		(layer "F.Cu")
		(uuid "733afa41-6f22-4281-83a5-959d324ff146")
		(at 112.464004 71.014004)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2 ISO7380")
		(property "Reference" "H1"
			(at 0 -2.7 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7f51f040-a50b-4687-9e77-beeb9bcdc18a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole"
			(at 0 2.7 0)
			(layer "F.Fab")
			(uuid "f7beac50-8e5a-4522-9226-1de4ae3ecc8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7e2e48e-8922-4780-99f3-62ffb4ceb257")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f7397dc-8467-489d-9479-563ca669a961")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*")
		(path "/3a84bd51-7348-4b73-b6e1-753bc992f741")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "1c84d89f-fd0b-421f-9356-4aab98003ba5")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "51719851-aae0-43b1-b0cc-62f7253ea118")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9a02dd5d-6b17-4cc2-9608-abd53c6a8e73")
			(effects
				(font
					(size 0.88 0.88)
					(thickness 0.13)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(uuid "3bc480ef-116b-4a2b-9892-631d86aba14f")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(uuid "7c65fdd8-3093-4fc2-8188-583a7237d78d")
		(at 76.85 108 180)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "95aaabba-50c0-4747-9cac-258f67497726")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "INA180A3"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "bb5fd4ee-c60e-4e96-a802-6ddcb715f57d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina180.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f2ca213-be3e-4b9e-8b92-559e8fd5031d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Current Sense Amplifier, 1 Circuit, Rail-to-Rail, 26V, Gain 100 V/V, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc0fe841-78fa-4cf4-a4ce-b38aed74b680")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/7aeb3891-57ce-4341-bf7e-eae1a367d539")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.91 1.56)
			(end -0.91 1.559999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "557ed260-9b58-4ae9-aa5c-ca36e3bef1e0")
		)
		(fp_line
			(start 0.91 1.51)
			(end 0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "903762ef-5dce-4626-9305-21583abd2296")
		)
		(fp_line
			(start 0.91 -0.39)
			(end 0.909999 0.389999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92e5fd7a-6f37-496f-8627-480aa804abe5")
		)
		(fp_line
			(start 0.91 -1.559999)
			(end 0.91 -1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a698020e-d6c5-441d-8b87-c25c316a0f3b")
		)
		(fp_line
			(start -0.91 1.559999)
			(end -0.91 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be5d055d-d1f8-4927-8c47-0f5f1b9975a1")
		)
		(fp_line
			(start -0.91 -1.51)
			(end -0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49423ccc-f47b-476e-88f0-388e64a92c4f")
		)
		(fp_line
			(start -0.91 -1.56)
			(end 0.91 -1.559999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16b8ab02-db03-4138-bac8-a2d64d48f8df")
		)
		(fp_poly
			(pts
				(xy -1.45 -1.51) (xy -1.69 -1.839999) (xy -1.21 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "e672d92c-c1bf-41a1-baf6-b209f8479bab")
		)
		(fp_line
			(start 2.05 1.5)
			(end 1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e8d9ddd-3e73-4325-81f9-3bc17b221a0b")
		)
		(fp_line
			(start 2.05 -0.39)
			(end 1.05 -0.39)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a382e1b2-312f-4f89-8c93-b4fef1f5b0a2")
		)
		(fp_line
			(start 2.05 -1.5)
			(end 2.05 -0.39)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2dcfe0e7-2515-4fc3-b0eb-d5bd51fb435e")
		)
		(fp_line
			(start 2.049999 0.389999)
			(end 2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a3aef51-8256-48af-91e1-0ed0ce92d42a")
		)
		(fp_line
			(start 1.050001 1.700001)
			(end -1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d26744e1-a81f-43e4-a6fd-8089b6a65da1")
		)
		(fp_line
			(start 1.05 1.5)
			(end 1.050001 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70512e81-89b1-45bf-a58f-eea7e187e8f4")
		)
		(fp_line
			(start 1.05 -0.39)
			(end 1.049999 0.39)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc40a044-8086-45ca-9bfc-9fcb0dfecef9")
		)
		(fp_line
			(start 1.05 -1.7)
			(end 1.049999 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7644824-bae9-4f00-839c-01ca0c923398")
		)
		(fp_line
			(start 1.049999 0.39)
			(end 2.049999 0.389999)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63bf01fc-e493-4c44-ab36-c630004b8c76")
		)
		(fp_line
			(start 1.049999 -1.5)
			(end 2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bb54e4d-9106-49f6-87f2-50bc6af1a6f1")
		)
		(fp_line
			(start -1.049999 1.5)
			(end -2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0565f2c-5bdc-467f-ba5b-66220a35db64")
		)
		(fp_line
			(start -1.05 1.7)
			(end -1.049999 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0aa1b81-cb61-4c66-8dc9-c27a698128fa")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.050001 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf6f8f8f-9290-4514-9b83-234890d0ed9e")
		)
		(fp_line
			(start -1.050001 -1.700001)
			(end 1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "771484dd-0612-4d53-8385-d1da51b5ae54")
		)
		(fp_line
			(start -2.05 1.5)
			(end -2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12e84eef-cd5b-4c3e-8900-98074cd25340")
		)
		(fp_line
			(start -2.05 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09eb64b7-30cc-4edd-a5f6-6976f20643a5")
		)
		(fp_poly
			(pts
				(xy -0.4 -1.45) (xy 0.8 -1.45) (xy 0.8 1.449999) (xy -0.8 1.45) (xy -0.799999 -1.05)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e539f9ca-49ce-4310-9ae8-56a97bbe5b00")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "3b07e84b-f3b5-4e4e-bf3f-56f127b32f45")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(R4-Pad1)")
			(pintype "output")
			(uuid "8cf216f1-23ac-445b-bca0-13820a4238db")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ba56b78e-eb48-445d-9952-d8733a29e92c")
		)
		(pad "3" smd roundrect
			(at -1.137499 0.949999 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "+12V")
			(pinfunction "+")
			(pintype "input")
			(uuid "25aa66ef-cbd2-4660-9bd7-d129e66b496e")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/BOUT_P")
			(pinfunction "-")
			(pintype "input")
			(uuid "cfcdc08e-3bf6-430b-9c35-8f59e0bb06bd")
		)
		(pad "5" smd roundrect
			(at 1.137499 -0.949999 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+3.3V")
			(pinfunction "V+")
			(pintype "power_in")
			(uuid "ac58d14d-8958-4f91-87fc-dbb8a497f6c8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(uuid "8689ed54-66e6-41ef-83a5-726a9ac85e94")
		(at 64.75 68.75)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J5"
			(at 1 -2.9 0)
			(layer "F.SilkS")
			(uuid "fae34ae1-ff10-4807-8d47-29e58bc15c48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5V_IN"
			(at 1 4 0)
			(layer "F.Fab")
			(uuid "f20e0c99-8cbe-4ead-8404-9923449a475a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0a09eeb-7650-4308-9202-476921a0656f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d07c546b-7cd5-482c-9df5-5f349fc58250")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/59dacb98-5a5c-45b6-8b97-c37915c63535")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.36 -2.11)
			(end -2.36 -0.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9723d4d5-396c-42a1-8039-c8ed27302d27")
		)
		(fp_line
			(start -2.06 -0.5)
			(end -1.45 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee14f2aa-5625-49b6-b21a-34d8a986136a")
		)
		(fp_line
			(start -2.06 0.8)
			(end -1.45 0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "594c9b85-5819-4e0d-9dd5-721cb57fc351")
		)
		(fp_line
			(start -1.45 -1.2)
			(end -1.45 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00fccac1-f719-409a-9996-c3d6f1e99a64")
		)
		(fp_line
			(start -1.45 2.3)
			(end 3.45 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99690133-a8ff-4c0f-b495-c7f63b772721")
		)
		(fp_line
			(start -1.11 -2.11)
			(end -2.36 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45e59738-bacf-40dc-8e90-0185143e2bb5")
		)
		(fp_line
			(start -0.6 -2.01)
			(end -0.6 -1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6019994-077a-4109-ae52-3809bc1b5808")
		)
		(fp_line
			(start -0.3 -2.01)
			(end -0.6 -2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9692975-697e-47be-b4ce-4f70c9cc387d")
		)
		(fp_line
			(start -0.3 -1.91)
			(end -0.6 -1.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "400d0494-484c-436e-9c4a-8d25df39e57d")
		)
		(fp_line
			(start -0.3 -1.81)
			(end -0.3 -2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efa1ecdb-d5e2-4fbd-8a04-fb4120f5b2c6")
		)
		(fp_line
			(start 0.5 -1.81)
			(end 0.5 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea0a72ee-6a98-4790-a8ee-40c76a604df8")
		)
		(fp_line
			(start 0.5 -1.2)
			(end -1.45 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1aaad757-015b-4f3a-a1a0-da0d50c51ef8")
		)
		(fp_line
			(start 0.9 1.8)
			(end 1.1 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e1e838f-7aec-4643-86a4-060465a9205d")
		)
		(fp_line
			(start 0.9 2.3)
			(end 0.9 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc480303-ba5f-4e06-bb1e-033c5c4d4cd3")
		)
		(fp_line
			(start 1 2.3)
			(end 1 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb5d0eb3-1e22-4ff2-8b7c-6175f88dd169")
		)
		(fp_line
			(start 1.1 1.8)
			(end 1.1 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad963d7b-bc73-4fad-8283-bcd75554270f")
		)
		(fp_line
			(start 1.5 -1.2)
			(end 1.5 -1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a1b9ad7-8537-44d6-8c04-acf6ec211353")
		)
		(fp_line
			(start 3.45 -1.2)
			(end 1.5 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "030ebd5c-5af7-4618-909f-7b6ffad0159b")
		)
		(fp_line
			(start 3.45 2.3)
			(end 3.45 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aebadd6c-c434-4798-b37f-d80e0e50e2c3")
		)
		(fp_line
			(start 4.06 -0.5)
			(end 3.45 -0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25bde0ff-44be-4620-8c2c-5cdd4646b5bf")
		)
		(fp_line
			(start 4.06 0.8)
			(end 3.45 0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9aaf600-5b6b-4b4d-8ac5-6c4192da1253")
		)
		(fp_rect
			(start -2.06 -1.81)
			(end 4.06 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "cafd7216-5a82-4aae-808e-9bc279e1d210")
		)
		(fp_rect
			(start -2.45 -2.2)
			(end 4.45 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "d2d20768-5afc-4f42-970f-c22787888244")
		)
		(fp_line
			(start -2.36 -2.11)
			(end -2.36 -0.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "040a6c39-350f-4221-97e1-dd43b6d63eb4")
		)
		(fp_line
			(start -1.11 -2.11)
			(end -2.36 -2.11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27bb66db-7e71-47a8-96c6-e9efae019585")
		)
		(fp_rect
			(start -1.95 -1.7)
			(end 3.95 2.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d293cab5-e835-4747-b2a7-bccf5db6614a")
		)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
			(uuid "6832e891-b2b1-4545-85ed-6948da274c65")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 35 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2881c3ac-1b70-43de-9fd2-bb6c0252ab75")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b7c7389a-6689-492c-96d1-f00de18c5e51")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "898c411f-b437-4d19-84e9-938767d49b66")
		(at 319.797499 3.625)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dce853cc-8959-4923-ba3a-8452bb201f30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS22917DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "888548a9-b16a-4a5a-a353-4c1b18bcc1dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps22917.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8233f0bd-56b2-42c3-af2d-d8d16e61cb45")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1V to 5.5V, 2A, 80mΩ Ultra-Low Leakage Load Switch, SOT23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5edfb48a-eb89-49dc-bf05-4e0c94577a07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/d10fe0f8-3b7f-4de1-b0fd-87c2ecdff6c4")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.91 -1.56)
			(end 0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c9d8b2c-88c6-47cd-804b-47ee95d36661")
		)
		(fp_line
			(start -0.91 -1.51)
			(end -0.91 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c0e2109-7161-43e3-8696-20669eb7e8dc")
		)
		(fp_line
			(start -0.91 1.56)
			(end -0.91 1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42458143-75da-4e66-b4e6-a699e87f00f5")
		)
		(fp_line
			(start 0.91 -1.56)
			(end 0.91 -1.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95c49f77-6257-4cec-b5f7-aa38a3ce72e8")
		)
		(fp_line
			(start 0.91 1.51)
			(end 0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "329e62d1-b971-4a65-bfe5-77d62ef1782a")
		)
		(fp_line
			(start 0.91 1.56)
			(end -0.91 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58e134a2-f8e8-43e3-bfff-6bf339bcf8ab")
		)
		(fp_poly
			(pts
				(xy -1.45 -1.51) (xy -1.69 -1.84) (xy -1.21 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "5a9dba33-5924-452d-8bf6-06c5377753fc")
		)
		(fp_line
			(start -2.05 -1.5)
			(end -1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b866f2ff-d1dd-44ed-b37f-a94fe86fa140")
		)
		(fp_line
			(start -2.05 1.5)
			(end -2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04562395-e42e-4353-bca8-5c4fae364db1")
		)
		(fp_line
			(start -1.05 -1.7)
			(end 1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f272880-d628-4924-9c91-a7f409b31dab")
		)
		(fp_line
			(start -1.05 -1.5)
			(end -1.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "add4e578-2deb-4342-b05b-0e27984c9edc")
		)
		(fp_line
			(start -1.05 1.5)
			(end -2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9590f080-ca6b-4d77-920b-04e5cb623d86")
		)
		(fp_line
			(start -1.05 1.7)
			(end -1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fca2a25-5865-4ee6-b263-a74edbdad736")
		)
		(fp_line
			(start 1.05 -1.7)
			(end 1.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9499b005-bfb4-4400-9d03-d58af84c4305")
		)
		(fp_line
			(start 1.05 -1.5)
			(end 2.05 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2004b1a4-1d56-4ddf-885d-5b57e74bfd59")
		)
		(fp_line
			(start 1.05 1.5)
			(end 1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a04b1a08-974d-4fb7-9552-3e24b48b15be")
		)
		(fp_line
			(start 1.05 1.7)
			(end -1.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d338a6a7-5ca8-468e-a214-58bdaeb49de0")
		)
		(fp_line
			(start 2.05 -1.5)
			(end 2.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72ec2533-bfde-413a-9e58-00a9e081c960")
		)
		(fp_line
			(start 2.05 1.5)
			(end 1.05 1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6279e27-ec2a-4c1c-a82f-a908c8506040")
		)
		(fp_poly
			(pts
				(xy -0.4 -1.45) (xy 0.8 -1.45) (xy 0.8 1.45) (xy -0.8 1.45) (xy -0.8 -1.05)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8ac7c5bc-646b-4e50-8399-4492e2c854cd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "195c5ae7-e5e4-455b-a04f-d11ad394b89e")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.11)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+3.3V")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "022e58b1-f520-4128-93af-8a8b9e9d6b0a")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "591bcf1d-f842-470e-93a7-0be47ea1b30d")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/DET_B")
			(pinfunction "ON")
			(pintype "input")
			(uuid "1a477b09-ed0c-4375-820b-f6d5cdf26956")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U2-CT-Pad4)")
			(pinfunction "CT")
			(pintype "output+no_connect")
			(uuid "ed18275c-bc58-4836-be53-8f18b8f30497")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(U2-QOD)")
			(pinfunction "QOD")
			(pintype "open_collector")
			(uuid "b284effa-b555-43e6-93c7-d92f6308f069")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "Net-(J10-VDD)")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "2aca3e64-03ca-49a8-8c33-9e45fdab308e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8a2fe830-05ed-4763-bb9a-524be54bdd64")
		(at 77.05 113.2 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ad5d010a-c8da-4740-bdb1-d894e8e15dd2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d3398698-948c-4d29-9bf6-4b821cb1db5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d52eba77-e949-40b9-bcb2-68fed7454e21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2e870d4-e4d0-46e3-b8a0-d159ce6a57d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/d04bd025-5a1e-4551-ab56-d2f2a5867f90")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "360077f8-c8f9-4a3d-b0cd-781a25f26052")
		)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ecea5ea6-976c-42a5-9661-94f27bd25f94")
		)
		(fp_poly
			(pts
				(xy -1.879999 -0.98) (xy 1.88 -0.98) (xy 1.879999 0.98) (xy -1.88 0.98)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b2eede0b-8f28-4626-9f45-d0d268701be9")
		)
		(fp_poly
			(pts
				(xy -1 -0.625) (xy 1 -0.625) (xy 1 0.625) (xy -1 0.625)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8c7e6b1a-66a2-4a49-8c94-d92f3eb815b2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e5b1efd9-174f-4f57-835c-9299331a835f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "/VBAT_ADC")
			(pintype "passive")
			(uuid "a218785c-0cb5-441b-8951-4cd3606a51a8")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "48cf62dc-3cad-40f0-8003-e170e5374ebc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a3ccc39c-4826-417c-903a-4a15a164b4c9")
		(at 319.25 -5.2 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dc50691a-6d90-4a8b-996c-33c97cb95950")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4829b42e-6305-4312-8800-b9d6af40cb94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "94b61ef8-49f5-403c-afdb-ce6cad322333")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "72df63d7-ba73-4af2-87d1-a6d42c74a574")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d172fae3-dba5-4929-887a-e5901b1e1a7c")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2a07fba-aa85-454d-a91b-f61c9d030f76")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6f126f2-b10b-4062-981a-1ec3c2efeb8f")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4f37536c-c0c5-48b1-b3e7-5ed32e725ed4")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "77a00d45-80e0-4604-98ea-0951c738d404")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "964ed0cb-b044-41a9-b0f4-fe2e152071f4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(J10-VDD)")
			(pintype "passive")
			(uuid "794e3983-3e91-4523-8983-e026391a7778")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Net-(J10-DAT1)")
			(pintype "passive")
			(uuid "d7e26348-b325-4f76-a663-bb9c9a2da86d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Card:microSD_HC_Molex_104031-0811"
		(layer "F.Cu")
		(uuid "b4f1dcb5-328b-4903-b1ad-4c2e1dd2d552")
		(at 333.55 -4.2)
		(descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
		(tags "microSD SD molex")
		(property "Reference" "J10"
			(at 0 -7.180001 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7147a736-0e72-4d72-b0fc-2b3726d9c630")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Micro_SD_Card_Det2"
			(at 0.000001 7.390001 0)
			(layer "F.Fab")
			(uuid "4dbce082-eca4-477c-96e2-b96d2172d2c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.hirose.com/en/product/document?clcode=&productname=&series=DM3&documenttype=Catalog&lang=en&documentid=D49662_en"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e1444e75-9898-4ee9-99da-ff23dcd2b33b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Micro SD Card Socket with two card detection pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "92c4d944-f916-47e4-ad73-8eab1a35d5d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "microSD*")
		(path "/5613a41b-9a51-483e-8ecb-0583993138cc")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.07 1.4)
			(end -6.069999 3.699999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ea72c3a-c6d0-4789-9420-5551117f98c3")
		)
		(fp_line
			(start -6.07 5.819999)
			(end -3.39 5.82)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8cb3a9d-feb2-4855-ab03-bd35dcca2fce")
		)
		(fp_line
			(start -6.069999 -4.45)
			(end -6.07 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4eddd424-d108-4d21-8a79-72a74a0a7936")
		)
		(fp_line
			(start -6.069999 5.1)
			(end -6.07 5.819999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ed8e7ac-847f-4945-bef4-6bbb994e4033")
		)
		(fp_line
			(start -4.59 -5.82)
			(end -3.730001 -5.82)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95ab352e-b8d9-4fa3-9482-1cf91897b131")
		)
		(fp_line
			(start -1.090001 5.820001)
			(end 2.58 5.82)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c792341-cd06-4246-91ae-31d2ad874f5d")
		)
		(fp_line
			(start 4.88 5.819999)
			(end 6.109999 5.820001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28ebf6f1-0449-4f85-8e7d-8043548e809e")
		)
		(fp_line
			(start 6.109999 5.820001)
			(end 6.11 -4.000001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "246ed20e-8e91-4206-8dcd-1674257f76a4")
		)
		(fp_line
			(start -6.840001 6.55)
			(end -6.84 -6.499999)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "796de337-9768-43cb-b76f-ec4bb6f4e0a2")
		)
		(fp_line
			(start -6.84 -6.499999)
			(end 6.840001 -6.499999)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bea906be-3bc1-441f-b7c2-529467fdf417")
		)
		(fp_line
			(start 6.84 6.55)
			(end -6.840001 6.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7ec39f8-beee-4176-8115-aca0018c2d26")
		)
		(fp_line
			(start 6.840001 -6.499999)
			(end 6.84 6.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd596600-cc3a-4061-8a06-8851d1829c2a")
		)
		(fp_line
			(start -5.955 -5.7)
			(end -5.954999 5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c719063-b825-433c-8935-d9bc7d8c831b")
		)
		(fp_line
			(start -5.955 -5.7)
			(end -4.26 -5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2e7c99a-8cdd-483c-8223-d1345d223eff")
		)
		(fp_line
			(start -5.405 -9.2)
			(end -5.405 -5.699999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b8be2aa-783c-4572-9577-152b13cd52b9")
		)
		(fp_line
			(start -4.905 -9.7)
			(end 5.095 -9.700001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbb8c56f-97a7-4d5f-88b9-3a6374df3d7a")
		)
		(fp_line
			(start -3.76 -4.8)
			(end -3.760001 -5.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed59b7d0-0f77-4361-b55c-3a4f9431caa6")
		)
		(fp_line
			(start 4.400001 -4.3)
			(end -3.260001 -4.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5eb541b2-86ea-4197-8317-b5d8fd4d6769")
		)
		(fp_line
			(start 4.899999 -5.400001)
			(end 4.899999 -4.799999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb09af01-cad8-4d01-968a-cbee61c66820")
		)
		(fp_line
			(start 5.595 -5.7)
			(end 5.594999 -9.200001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fed7762e-5ec5-4b8e-a43e-160ec24a4870")
		)
		(fp_line
			(start 5.994999 -5.7)
			(end 5.21 -5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "350c3dc5-ff59-47bb-b683-c550f51ab44e")
		)
		(fp_line
			(start 5.995 5.7)
			(end -5.954999 5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0dec9e1c-e30e-4f3f-96d8-36d2766762df")
		)
		(fp_line
			(start 5.995 5.7)
			(end 5.994999 -5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8823a6d2-dd6b-4161-9c05-08ef1dc8e497")
		)
		(fp_arc
			(start -5.405 -9.2)
			(mid -5.258554 -9.553553)
			(end -4.905 -9.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ad091e3-9cf7-4d7d-b229-edc4d41584e3")
		)
		(fp_arc
			(start -4.26 -5.7)
			(mid -3.906447 -5.553553)
			(end -3.760001 -5.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "feec8c0f-236d-4de3-9a1d-67c63e038896")
		)
		(fp_arc
			(start -3.260001 -4.3)
			(mid -3.613554 -4.446448)
			(end -3.76 -4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2da8398-89a3-4ece-8acd-ac832328ae28")
		)
		(fp_arc
			(start 4.899999 -5.400001)
			(mid 4.987866 -5.612132)
			(end 5.199999 -5.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc107367-5483-4d47-bbbc-30bdc5ce7177")
		)
		(fp_arc
			(start 4.899999 -4.799999)
			(mid 4.753552 -4.446448)
			(end 4.400001 -4.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c935da2c-b655-41bc-bbde-38885b917110")
		)
		(fp_arc
			(start 5.095 -9.700001)
			(mid 5.448553 -9.553554)
			(end 5.594999 -9.200001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01f07452-c9ad-410b-9639-19da58a447e5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ec87df03-0223-4711-a5d8-7cf94de4a6f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.105 -5.449999)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(J10-DAT2)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
			(uuid "f83ba442-4746-4f30-b115-0cf75af3b76e")
		)
		(pad "2" smd rect
			(at -2.005 -5.449999)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/SD_CS")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
			(uuid "6a11360f-47a3-49c1-a7b8-3239be88c6c7")
		)
		(pad "3" smd rect
			(at -0.905001 -5.45)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SD_MOSI")
			(pinfunction "CMD")
			(pintype "input")
			(uuid "b0eeda12-3d2d-4b95-8946-9a2d05aa4c45")
		)
		(pad "4" smd rect
			(at 0.195001 -5.45)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(J10-VDD)")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "e7b865a1-c4d3-45de-b0f9-0dd62ea32866")
		)
		(pad "5" smd rect
			(at 1.295 -5.449999)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/SD_CLK")
			(pinfunction "CLK")
			(pintype "input")
			(uuid "6980a083-6153-4dc7-a693-17b496f4fffe")
		)
		(pad "6" smd rect
			(at 2.395001 -5.45)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "b426ab54-cd42-4224-a23b-bdc0465ff3f0")
		)
		(pad "7" smd rect
			(at 3.495001 -5.449999)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/SD_MISO")
			(pinfunction "DAT0")
			(pintype "bidirectional")
			(uuid "b9232792-2565-457b-878e-7b87fe2a5e59")
		)
		(pad "8" smd rect
			(at 4.544999 -5.45)
			(size 0.75 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(J10-DAT1)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
			(uuid "f600f602-1f4c-4a94-89fd-c826981ad8d3")
		)
		(pad "9" smd rect
			(at -5.74 0.700001)
			(size 1.2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "/DET_B")
			(pinfunction "DET_B")
			(pintype "passive")
			(uuid "3a94ac49-0786-4b7c-9118-1d6523d0b43e")
		)
		(pad "10" smd rect
			(at -5.74 4.4)
			(size 1.2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/DET_A")
			(pinfunction "DET_A")
			(pintype "passive")
			(uuid "569c4091-528f-4a5f-85d8-3ef139be1249")
		)
		(pad "11" smd rect
			(at -5.564999 -5.325)
			(size 1.55 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J10-SHIELD)")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "b25dfe63-4470-466c-866e-861c35b6e916")
		)
		(pad "11" smd rect
			(at -2.24 5.375)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J10-SHIELD)")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "0d54d4d1-d849-4900-ac13-8d093e867e1b")
		)
		(pad "11" smd rect
			(at 3.73 5.375001)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J10-SHIELD)")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "fd3d81ed-3ee8-4e34-a799-cba973f43522")
		)
		(pad "11" smd rect
			(at 5.755 -5.1)
			(size 1.17 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J10-SHIELD)")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "72c4ffe6-1eae-4eed-a35c-7e66f6d75c4a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Molex_104031-0811.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "cfb79710-fde0-4f48-9ad0-e140bfcb606e")
		(at 80.15 112.3 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6c0a4bdd-ab47-46e6-8606-310c2eb7e5bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "3058d8a2-53c5-441d-afab-ea57e3dd016f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b83c009c-9bd2-4430-a746-c83978080ead")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec47fd70-cd9a-4636-bcdd-bf579a38a4ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f2874c4b-00e7-4dfd-91c1-04c9cd8e58eb")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227065 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9c00a18-0844-4d0e-a28f-184af7909767")
		)
		(fp_line
			(start -0.227065 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "145c198d-7267-4dd1-8ed3-ad4d9366bec3")
		)
		(fp_poly
			(pts
				(xy -1.85 -0.95) (xy 1.85 -0.95) (xy 1.85 0.95) (xy -1.85 0.95)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ec71145c-eb0c-438e-9849-9b0959646642")
		)
		(fp_poly
			(pts
				(xy -1 -0.625) (xy 1 -0.625) (xy 1 0.625) (xy -1 0.625)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "af16b1af-9e5d-4b2c-8bd6-644826d1ce0f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6a678445-ec5a-4c2a-a03e-fdbaaaf77494")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.000001 -0.000001 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "/VBAT_ADC")
			(pintype "passive")
			(uuid "98b4f0c9-4371-4aa2-b9a4-8d11bc80beb1")
		)
		(pad "2" smd roundrect
			(at 1.000001 0.000001 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "GND")
			(pintype "passive")
			(uuid "c6be8677-3c78-4284-bac1-d87b27567398")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "d0b1663a-a4e6-4bf5-8c6f-ef9f5dec053d")
		(at 319.634999 6.325 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ffe6d1b2-b062-489b-8104-a6f6ac7e78db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1u"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d0ad2636-dd68-4ed3-beb0-0ff9261ec7b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "80028906-18b4-4b52-881d-b374f4248dfd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9564a6e8-51e4-4ccc-b325-d94a7188390a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3dd93a75-f2dd-4e1b-88e7-b8a69729b461")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "81434975-810f-4748-923d-b35a382d82b7")
		)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ca08504-76a6-494b-a17d-c5d79951004b")
		)
		(fp_rect
			(start -1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "9ec586e3-9a29-405b-bee2-66019a114a85")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d6e600b7-5390-4a98-8687-dddb558a01a7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6e8889e7-ef38-4b9e-89eb-10f64406d959")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 34 "/DET_B")
			(pintype "passive")
			(uuid "e79244d3-042f-4843-8973-77b70c9e4f3f")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "faf082c9-ab7a-4b5f-a1e0-305975c2e90e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "d62b7294-e960-42f4-b6a8-5e1d9c3de7a2")
		(at 316.684999 3.925 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "7c04b51e-4feb-4584-962b-335c329616c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "fa6d8156-1314-40f6-8cbc-8a1df265121b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4b6904f-9835-4e94-ace8-09d785df6263")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c12f35b4-a494-44d1-848c-e96277574679")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/28f76446-66fb-4912-bd8d-288238f0e3dd")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f252004e-d815-46fe-8786-21d909a9599c")
		)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a72a148b-1d4f-4e88-8769-07c049ff3e7b")
		)
		(fp_rect
			(start -1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c00b99de-690e-4fd7-9a52-7725da9722ee")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "460a2bf3-cbfc-4271-81e9-4e1219ca5c0e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "04287aa5-e48d-49f0-93a2-1a959e0898e6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "38067719-477e-4969-9f69-2302feace461")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "32dedc69-8482-4d1b-8e81-e9e5aa7a2bff")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "d8a04fb5-51f1-4960-be64-613198da22e9")
		(at 255.47 55.9)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "92d8514e-fb87-457d-a26d-7376614c8707")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.68 180)
			(layer "F.Fab")
			(uuid "37606718-c981-40dd-bafb-b5e5e5acc970")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "58363d2c-a88e-4cf4-9dad-472cee87bd07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "b98a3fa9-ab40-492a-b586-c4caf83a65c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/8d7210a4-e5aa-422e-bf0a-3be8bb608e12")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84bbac4d-b4cb-4f7b-853a-f7e8e4cd86a1")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39afbaef-b1c4-40b3-b314-09a09e513cfc")
		)
		(fp_rect
			(start -1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "595b4029-9e34-4df7-bc50-66567132c073")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3a9256ae-62a4-412a-b246-99bcc7f5342a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "e4827ac0-da03-4a34-aa41-722508342d3d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "0dc348bd-aaa5-4692-b96a-07c5d0693f72")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "097e5343-cdca-4e60-a969-a089db36828d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "daec386d-9d42-48b5-ad60-76f54b64b13f")
		(at 314.834999 10.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "580ad398-594a-4772-9482-dac199133980")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0b929a3e-1d28-44de-8073-9dfac206b2e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a249e401-dec8-4878-8bcf-21d338a2f736")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d11f6973-35f1-44fc-8a67-e754812bf1af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f4d05e08-0823-4452-9d04-790d3bec02b2")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "027ebee6-2691-459b-928d-83093e87134f")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a3beb2a-cdef-461e-a047-bd55b277176f")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "77a7e9f0-b8bb-454f-8485-baf1f25f8b8c")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "d0daf8e1-244f-43bd-98d7-0a685a224902")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "69549bdb-00b1-4aca-b98a-e040477f93d4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "f25c3653-dd77-4a7f-9f1a-8780bed90f83")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 38 "/DET_A")
			(pintype "passive")
			(uuid "d1cb340e-42de-4f66-afba-37f98f207cce")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "dfab939a-87a2-4d65-8973-f3182fefecf2")
		(at 225.35 80.7 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c957adf3-a40f-4778-8b6c-f913bd4e8d81")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "cb446af1-7f51-4d98-a6bc-cad262f5b1a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed85ceab-c865-4292-8d75-2c0e7231646f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4bf2dd4-e0d8-4b38-9c50-42882d316671")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2c786a0b-15d4-4a14-83f9-90e41e877b96")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35980d70-2c41-4ef1-ae4b-fec4bb34aadf")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "839bc1a6-2eb9-4d18-895d-1072f3d92299")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ee6f71a7-c0c3-490c-89e3-c8dc2580afd6")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1b5b344f-7091-4c74-8d74-e76d7f407481")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ee504604-d544-4915-aa0e-30b3684d8f33")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "39a98601-270f-4509-9da4-262be1d058d0")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "/NTC_ADC")
			(pintype "passive")
			(uuid "378c8c6a-12a5-479b-bd4d-7e4593c0a82e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e19dfa5d-085a-4cab-9421-87b793297ed2")
		(at 322.959999 3.525 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6a56f72a-002e-48ba-bb11-662d942ab28a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "712b8978-cf25-4745-856e-9ecf7ace13fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "59aebddb-b62f-4937-abd3-ac08715749a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "05ccf9a6-1978-40a8-b286-0ecb3cb609f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7184d09d-190c-4923-8bab-67316130036d")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42907b85-51c4-4457-917c-e2d0e7ca6da7")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78ff3786-8bba-436a-b4bc-2922946a3bdf")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "df1cbe91-f5b1-4b40-83aa-b834506ae784")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2935154c-aa73-4854-8adb-4f7b1dc507f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "09bca21b-c5ff-44f7-9375-8071c292cdff")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(J10-VDD)")
			(pintype "passive")
			(uuid "cb0915c5-83ce-4564-b93d-ac0fdc75c5cc")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 43 "Net-(U2-QOD)")
			(pintype "passive")
			(uuid "ca5009a7-b6ac-4bed-9760-8b8833331b63")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e9cc44ea-1dbb-4155-b30d-883c62cf0721")
		(at 255.47 59.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "28bc7c81-c8e0-4632-b0d7-c488ffb5a2a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "8b59c8a9-3be2-4426-8333-72a5d1fb5b62")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d45a8e8-8b53-4840-930a-8344c40da0da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2e05483-9b73-4cdc-bf56-2d85aef18be6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/d93c3a67-5738-4387-97dd-d80f59e9c6a8")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce0ed01f-e7bd-4eb0-8f63-a75a94bc95f3")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c20c781-03e3-41d6-ac8e-cd132059ecb2")
		)
		(fp_rect
			(start -1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1fe520bd-9c76-45f1-a2a1-ae3873293593")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "27b92cd0-f140-4ae4-aec1-13aef493019a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "646ea312-0734-4817-8ed7-57213dee824f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 27 "Net-(A1-ADC_VREF)")
			(pintype "passive")
			(uuid "81f1946c-8b69-4247-8220-4aa67db0e1f7")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "cfd04724-22a1-4e03-9f75-5570ebd81fff")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f5b6f29f-f766-4c74-8cce-37d00c69d2d4")
		(at 252.45 29.8929)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7b2e54f6-1181-44d8-b01a-fbb2274b31d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "cd32cc11-7c08-420a-b0db-3daf2ecc7ca0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7753d32f-8bc5-4587-afe6-0d4612463305")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eff5763c-217c-48d0-98df-a91139f2f92b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ca5f51f4-3a4e-405e-b897-680c85cbde74")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7827c732-ba2d-4e74-b139-a8107f12bfc8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa1f3298-06b5-49b5-87b8-f129ab842eee")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c44d084c-b7e6-4726-becf-601e992d22ab")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "44edb131-0dfd-447c-8a38-a86bc8d054b2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b34dd2c8-71bf-4c02-96bd-5e939d192be5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+3.3V")
			(pintype "passive")
			(uuid "144db7ab-deea-4dd6-af3a-5690c628bac5")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "/SCL")
			(pintype "passive")
			(uuid "15abb588-b0e1-43b5-85d5-9635621609be")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f86c2308-665d-4945-8f4f-a84c5e3cb839")
		(at 255.47 61.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2c29eacd-aed1-47c9-87b0-c33d55fa37ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "0d4ab7b7-2d02-479b-94f7-e9dd9e303b53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "55fd1ac7-bd90-4292-abbb-5d0681477dce")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "07aee070-952f-4bee-802c-7db6cca97458")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2a18e47d-224c-442f-8ecc-71b8cdbf1b09")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8bde1f8-d6d7-45cf-97c2-4c2c947dc2f8")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95e74e58-9933-4ede-87b1-a14c9e60f174")
		)
		(fp_rect
			(start -1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "7ee598fc-c3f4-4a47-ae2d-0cdb25e80e15")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b1463f95-bd3e-4789-8cb0-6ca08b509566")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2cbdd35a-586a-4974-81e1-fa1a465083c9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 27 "Net-(A1-ADC_VREF)")
			(pintype "passive")
			(uuid "c3e800fd-7174-49ea-848f-5c8cac1df65b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "GND")
			(pintype "passive")
			(uuid "d153062b-f63a-4c6d-996d-4136eb68f7d3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "HX711Module:HX711_Module_NoAnalog"
		(layer "B.Cu")
		(uuid "5d25560b-5e00-4905-aa79-ab00cd269cd5")
		(at 124.35 97.5 -90)
		(descr "Unnamed StepUp generated footprint")
		(property "Reference" "U3"
			(at 0 -1 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "a520175c-c197-4982-8a0d-6f6bdbb17e44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "HX711_Module_NoAnalog"
			(at -3 -6.3 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "47dab13b-4876-4a42-9908-8fd26f3b433c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "36453360-b32a-4e59-b1a6-51f82f3112f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "4bde0a9a-4f40-4cb7-bd5e-a3b3c571b0fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(path "/08980502-745f-466f-a652-6c48b9b3fd76")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -13.1 3.8)
			(end -12.4 4.5)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "B.SilkS")
			(uuid "816027f5-4a30-4538-ae38-9aea0320b209")
		)
		(fp_rect
			(start -13.1 4.5)
			(end -10.4 -5.5)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "9ac853ba-305d-42b2-bd57-9a74894081fc")
		)
		(fp_circle
			(center -11.8 7)
			(end -13.4 7)
			(stroke
				(width 0.16)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "e8701ddc-46b6-4171-ab70-985beafb1a22")
		)
		(fp_circle
			(center -11.8 -7.7)
			(end -13.4 -7.7)
			(stroke
				(width 0.16)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "ee04f5b8-3139-470f-b67a-ee9abe81f2c2")
		)
		(fp_poly
			(pts
				(xy -16.6 10.2) (xy 16.6 10.2) (xy 16.6 -10.2) (xy -16.6 -10.2)
			)
			(stroke
				(width 0.16)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "e4d8b1da-a1ad-443f-87c9-70cc62ad9e2c")
		)
		(fp_rect
			(start -13.15 4.5)
			(end -10.45 -5.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "79bd3c8a-59a3-4f90-b7f0-feafa609b1ae")
		)
		(fp_circle
			(center -11.8 7.027692)
			(end -12.8 8.727692)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "8c12abcd-c991-4225-9b2a-a629a582255b")
		)
		(fp_circle
			(center -11.8 -7.7)
			(end -12.8 -6)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "62b172cf-f527-4f03-98f6-02620c8eacf1")
		)
		(fp_text user "${REFERENCE}"
			(at -11.5 -11.5 90)
			(layer "B.Fab")
			(uuid "00a6e5b7-9ecf-4b88-a2b4-926e90f30f57")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole circle
			(at -11.8 3.273 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "29b830db-924c-4d44-8eea-931d39ef2747")
		)
		(pad "2" thru_hole circle
			(at -11.8 0.733 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/LC_DT")
			(pinfunction "DT")
			(pintype "bidirectional")
			(uuid "eec0745d-159b-4a8a-8178-b44f7d298814")
		)
		(pad "3" thru_hole circle
			(at -11.8 -1.807 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/LC_SCK")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "c770e40e-e235-4be4-9690-f56e0e8db892")
		)
		(pad "4" thru_hole circle
			(at -11.8 -4.347 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "999e2680-98a7-48c2-bef1-66fee03f80b6")
		)
		(embedded_fonts no)
		(model "/home/ale/Documents/Uni/Leaning/Unnamed.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_AMASS:AMASS_XT60-F_1x02_P7.20mm_Vertical"
		(layer "B.Cu")
		(uuid "60bfb004-b3fb-4226-9d5c-5e782669a5ed")
		(at 69.35 111.5 90)
		(descr "AMASS female XT60, through hole, vertical, https://www.tme.eu/Document/2d152ced3b7a446066e6c419d84bb460/XT60%20SPEC.pdf")
		(tags "XT60 female vertical")
		(property "Reference" "J3"
			(at 3.6 5.299999 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "ab8085d9-ef5a-470a-9305-d89c1b3ca71a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "BAT_OUT"
			(at 3.600001 -5.4 90)
			(layer "B.Fab")
			(uuid "8cd61475-f46c-4029-8293-dfaeb90d4735")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d94f1cb3-0e5b-497b-85b3-20f48355cd3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "664319ca-faaa-4ea3-8bf2-90cee09eb3ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/2e179eaa-88d4-4e1f-8720-2fefdfd6bc84")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 11.45 -4.15)
			(end 11.45 4.150001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "42afbe98-e6df-4ab8-bef6-1d03d70997b2")
		)
		(fp_line
			(start -1.4 -4.149999)
			(end 11.45 -4.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fa1cd48a-57b3-4351-9289-0144723df779")
		)
		(fp_line
			(start -4.25 -1.55)
			(end -1.4 -4.149999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "27dcb555-014a-425d-a1f8-35530f6f667a")
		)
		(fp_line
			(start -4.25 1.6)
			(end -4.25 -1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "49e63386-4755-40f1-9ec3-3e2cc3fca613")
		)
		(fp_line
			(start 11.45 4.150001)
			(end -1.4 4.150001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "07bb2578-07a0-4f8f-90c3-d7f44c39b99c")
		)
		(fp_line
			(start -1.4 4.150001)
			(end -4.25 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9d346225-7a60-4df9-92e5-84eda760a762")
		)
		(fp_line
			(start 11.85 -4.6)
			(end -1.6 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2621dbd7-c73b-42de-8353-3f09fb7468d0")
		)
		(fp_line
			(start -1.6 -4.6)
			(end -4.65 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "49f5eeb3-4c62-4cd4-9bd0-e7ae6d17f798")
		)
		(fp_line
			(start -4.65 -1.85)
			(end -4.65 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "82397200-47c5-4c93-9c75-02ba0e801099")
		)
		(fp_line
			(start -4.65 1.85)
			(end -1.6 4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d2bebd44-3d0c-4a3e-9f7b-b0cb32bd552a")
		)
		(fp_line
			(start 11.85 4.6)
			(end 11.85 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "96490955-9b8f-431f-9e5d-0bf938bc372f")
		)
		(fp_line
			(start -1.6 4.6)
			(end 11.85 4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d5f15e56-c698-4202-b38f-89d5bdbe629e")
		)
		(fp_line
			(start 11.350001 -4.05)
			(end 11.35 4.049999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f23a4ced-e0f8-45db-a8e9-c5fc224ff08c")
		)
		(fp_line
			(start -1.399999 -4.05)
			(end 11.350001 -4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0f50185c-a5ae-4116-a784-7bce296c9f44")
		)
		(fp_line
			(start -4.150001 -1.55)
			(end -1.399999 -4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ce97726c-f024-44fd-95f3-ae07b32b50b4")
		)
		(fp_line
			(start -4.149999 1.55)
			(end -4.150001 -1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dc52f651-6325-477e-8a3a-478ee00afcdd")
		)
		(fp_line
			(start 11.35 4.049999)
			(end -1.4 4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f02b73a3-1dcb-4bfe-921d-258121bace72")
		)
		(fp_line
			(start -1.4 4.05)
			(end -4.149999 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7425ef06-7c91-4dc9-8ffc-b7a6515bf8a5")
		)
		(fp_text user "${REFERENCE}"
			(at 3.599999 -0.05 90)
			(layer "B.Fab")
			(uuid "300512ba-3441-4382-a794-a36e955d8252")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 6 6)
			(drill 4.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "bec55f8f-e038-48e6-894d-b9e7608012c2")
		)
		(pad "2" thru_hole circle
			(at 7.2 0 90)
			(size 6 6)
			(drill 4.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/BOUT_P")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "05041d27-a189-4fca-a101-259410b73ac4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT60-F_1x02_P7.2mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_AMASS:AMASS_XT60-F_1x02_P7.20mm_Vertical"
		(layer "B.Cu")
		(uuid "6119f05f-ceb4-4f15-8c74-71aafaec6d36")
		(at 84.45 111.499998 90)
		(descr "AMASS female XT60, through hole, vertical, https://www.tme.eu/Document/2d152ced3b7a446066e6c419d84bb460/XT60%20SPEC.pdf")
		(tags "XT60 female vertical")
		(property "Reference" "J2"
			(at 3.6 5.299999 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "fc74fc72-0d5a-4615-94c0-9b01786a14ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "BAT_IN"
			(at 3.600001 -5.4 90)
			(layer "B.Fab")
			(uuid "d3b52058-3c32-4832-85d0-27a5ddabf7d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f4dc4705-8a49-4c5a-8a35-8dfd8d013513")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4800bf30-76b1-4dcc-b960-470d4b4cbc0c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/a662108c-dd4b-429a-83aa-5e4f45aac7d4")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 11.45 -4.15)
			(end 11.45 4.150001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a4158bae-38cc-499a-bbc5-2d8b6eddad88")
		)
		(fp_line
			(start -1.4 -4.149999)
			(end 11.45 -4.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c94dfedd-bbfb-462d-ba83-77668ff51d2d")
		)
		(fp_line
			(start -4.25 -1.55)
			(end -1.4 -4.149999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d33062e5-3a9e-4bf7-baee-9d4ccf94a9ec")
		)
		(fp_line
			(start -4.25 1.6)
			(end -4.25 -1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f8da29df-826f-4857-b2da-dd32d4751535")
		)
		(fp_line
			(start 11.45 4.150001)
			(end -1.4 4.150001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "457cbdd1-7755-4532-ae48-b2d1820abd4f")
		)
		(fp_line
			(start -1.4 4.150001)
			(end -4.25 1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ccb3e8f7-fd3e-484f-a75f-e7c4c7473e1e")
		)
		(fp_line
			(start 11.85 -4.6)
			(end -1.6 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c1af4b12-d4c5-41c9-8ac9-df46960b6d30")
		)
		(fp_line
			(start -1.6 -4.6)
			(end -4.65 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "73b8d03c-ea14-4e0c-96b3-c9331d9f6e09")
		)
		(fp_line
			(start -4.65 -1.85)
			(end -4.65 1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "89b65b40-9253-4abf-99a3-c6e84d91d1ce")
		)
		(fp_line
			(start -4.65 1.85)
			(end -1.6 4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1ed67198-dbd6-4571-9394-745687cbe4db")
		)
		(fp_line
			(start 11.85 4.6)
			(end 11.85 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "20375e45-790c-45a8-bd23-b57f70de60ab")
		)
		(fp_line
			(start -1.6 4.6)
			(end 11.85 4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "007612a2-41ec-436b-9440-6d1408c5903b")
		)
		(fp_line
			(start 11.350001 -4.05)
			(end 11.35 4.049999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "71a877ff-04cc-4e47-9bb6-389a8b32c88c")
		)
		(fp_line
			(start -1.399999 -4.05)
			(end 11.350001 -4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "40a516b8-c125-4e96-ad58-47f18f5a8f87")
		)
		(fp_line
			(start -4.150001 -1.55)
			(end -1.399999 -4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "983cbc2e-c615-47d2-bd9f-9444a86b3621")
		)
		(fp_line
			(start -4.149999 1.55)
			(end -4.150001 -1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "50cd732d-4a76-47f7-8067-163de371c553")
		)
		(fp_line
			(start 11.35 4.049999)
			(end -1.4 4.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "152bcb35-2990-4d73-bb12-352e08cf0eb6")
		)
		(fp_line
			(start -1.4 4.05)
			(end -4.149999 1.55)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "94e4fb17-b19d-40e0-90ed-dcb223e8926d")
		)
		(fp_text user "${REFERENCE}"
			(at 3.599999 -0.05 90)
			(layer "B.Fab")
			(uuid "ebc3ebf7-d526-4890-82ed-c3fb09c88565")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 6 6)
			(drill 4.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "a0322d93-7aa3-4d49-93d7-469cb8324838")
		)
		(pad "2" thru_hole circle
			(at 7.2 0 90)
			(size 6 6)
			(drill 4.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "+12V")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "5451c292-ea3d-4cd4-a03f-5bb1f63aaff9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT60-F_1x02_P7.2mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical"
		(layer "B.Cu")
		(uuid "c18b93b2-7945-4a02-ac7d-b293256a84c1")
		(at 272.349999 76.499999 180)
		(descr "JST PH series connector, B4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J4"
			(at 3.000001 2.900001 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "04605080-4658-4cba-bd7a-c9e452b66c7d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "PITOT"
			(at 2.999999 -4 0)
			(layer "B.Fab")
			(uuid "fe4f37b0-0382-416a-ac3a-8ebf8d20821d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "54d28258-de31-4e91-a301-692f937d4726")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "6950b64f-617d-450f-8939-f241da649ff9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/232dcb86-d003-4034-82ca-5e74f36d90d6")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.06 0.5)
			(end 7.450001 0.499999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a5f3aad7-a4da-4f6f-81cf-f46fccc15bf7")
		)
		(fp_line
			(start 8.06 -0.799999)
			(end 7.450001 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d72f0cd6-379a-49b2-ad0a-628d48d81645")
		)
		(fp_line
			(start 7.45 1.199999)
			(end 5.5 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "380294fb-df66-42b7-85a8-a85c59b72196")
		)
		(fp_line
			(start 7.449999 -2.299999)
			(end 7.45 1.199999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c7643b5b-a3a3-455a-8a3c-7bbf780a83cf")
		)
		(fp_line
			(start 5.5 1.2)
			(end 5.5 1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4e8d4416-f953-4b97-bf12-9055a6f5a24e")
		)
		(fp_line
			(start 5.100002 -1.8)
			(end 5.1 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6cb30da8-33c3-4f2f-91fd-5c2fbab98699")
		)
		(fp_line
			(start 5.000001 -2.299998)
			(end 5.000001 -1.800001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "16117d93-6bdd-46d1-8b06-1775466e7c09")
		)
		(fp_line
			(start 4.9 -1.800001)
			(end 5.100002 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8e8f7f43-d71f-419a-9010-ba1383c4b04b")
		)
		(fp_line
			(start 4.9 -2.3)
			(end 4.9 -1.800001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7fe722d7-0d0c-4a25-94cb-92e5fb0832f7")
		)
		(fp_line
			(start 3.1 -1.800001)
			(end 3.100001 -2.299999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d976ddee-e048-4c24-942e-f542ed8662c7")
		)
		(fp_line
			(start 3 -2.299999)
			(end 2.999999 -1.800001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "eee8c99b-a617-40df-b9af-bbbd049d9619")
		)
		(fp_line
			(start 2.9 -1.8)
			(end 3.1 -1.800001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "08f37bd4-bbaf-4490-9932-c940f856a2d4")
		)
		(fp_line
			(start 2.9 -2.299999)
			(end 2.9 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0545cbbb-cdf0-4de3-991a-d36cca1126de")
		)
		(fp_line
			(start 1.1 -1.8)
			(end 1.100001 -2.299999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "34605c9f-0bc6-4d4b-b8f3-96d5bcbe278f")
		)
		(fp_line
			(start 0.999999 -2.299999)
			(end 1 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0cacc89f-ec11-42f8-9411-5ac51671fc86")
		)
		(fp_line
			(start 0.9 -1.8)
			(end 1.1 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0ca57786-79d1-43fd-aaa0-f6f9d73d4d34")
		)
		(fp_line
			(start 0.9 -2.299999)
			(end 0.9 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4f149ba0-7bba-4369-a2b2-af8346bf7074")
		)
		(fp_line
			(start 0.499999 1.809999)
			(end 0.499999 1.199999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0f516500-8217-41e4-92e7-2a5f2b7cfc6c")
		)
		(fp_line
			(start 0.499999 1.199999)
			(end -1.450001 1.199999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ef147779-373a-4e1b-a0ef-8e476f6c9744")
		)
		(fp_line
			(start -0.300001 2.01)
			(end -0.6 2.010001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "86d2c761-3164-4d29-ac3e-31395e1403cc")
		)
		(fp_line
			(start -0.300001 1.91)
			(end -0.599999 1.910001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c51df155-c15f-4911-84f3-1e8c001d8001")
		)
		(fp_line
			(start -0.300001 1.81)
			(end -0.300001 2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8bb353bd-879f-4dfa-9351-b7989aa85cb0")
		)
		(fp_line
			(start -0.6 2.010001)
			(end -0.599999 1.810001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e3afe092-5e0b-46e6-ba9e-b5fd9890b1e1")
		)
		(fp_line
			(start -1.110001 2.11)
			(end -2.359999 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f3eab961-0562-4b22-8c42-da0023932e48")
		)
		(fp_line
			(start -1.449998 -2.299999)
			(end 7.449999 -2.299999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "22dcb87e-c433-43e9-ab78-fdf7e4fcca1e")
		)
		(fp_line
			(start -1.450001 1.199999)
			(end -1.449998 -2.299999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "83e744a2-6ce3-4004-a4d1-2918d241f2a9")
		)
		(fp_line
			(start -2.059999 0.5)
			(end -1.449999 0.499999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c6a0c40a-9373-45f8-930c-c62ec1367f89")
		)
		(fp_line
			(start -2.06 -0.8)
			(end -1.449999 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d9f257f5-2cc0-4d28-900e-aa99a765765c")
		)
		(fp_line
			(start -2.359999 2.11)
			(end -2.36 0.859999)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "96d0414a-2987-41cb-9ffd-2fe5c2c851bb")
		)
		(fp_poly
			(pts
				(xy -2.06 1.81) (xy -2.059999 -2.91) (xy 8.059999 -2.910001) (xy 8.059998 1.81)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "6b9c1505-8a30-497b-8a6e-1f0040c98b07")
		)
		(fp_poly
			(pts
				(xy -2.449999 2.2) (xy -2.449999 -3.300001) (xy 8.449999 -3.3) (xy 8.450001 2.200001)
			)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "a5584fff-9052-429b-acb5-d1ed4eea1c31")
		)
		(fp_line
			(start -1.110001 2.11)
			(end -2.359999 2.11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "535251c1-16ea-42ee-b8ee-b8571c9d32f0")
		)
		(fp_line
			(start -2.359999 2.11)
			(end -2.36 0.859999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "452b6ab8-0b52-4ce2-873c-fc50978251f0")
		)
		(fp_poly
			(pts
				(xy -1.95 1.7) (xy -1.95 -2.799999) (xy 7.950001 -2.800001) (xy 7.95 1.7)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "44f135fb-fd42-4e95-ac39-5eabe008c348")
		)
		(fp_text user "${REFERENCE}"
			(at 3 -1.5 0)
			(layer "B.Fab")
			(uuid "fa63269e-5cf5-44c3-b0ca-37fb1a9f5e2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 14 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "50502ce8-5e22-402a-a685-8b646f746bf7")
		)
		(pad "2" thru_hole oval
			(at 2 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b542f877-535a-4fa8-a08b-1a953238932e")
		)
		(pad "3" thru_hole oval
			(at 4.000001 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "a9bec98c-18d4-4b56-b618-4e72078085bb")
		)
		(pad "4" thru_hole oval
			(at 5.999999 -0.000001 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "f767a541-5522-4eb2-a04b-cb444419568e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(uuid "cddb56b3-c47a-4c08-bcf8-6ee47f79452e")
		(at 274.147974 81.736673 180)
		(descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x03 2.54mm single row")
		(property "Reference" "J6"
			(at 0 2.77 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "83669dc2-4a0e-4954-af85-5806696d1a95")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "RPM SENS"
			(at 0 -7.85 0)
			(layer "B.Fab")
			(uuid "d174ae94-4e92-42fb-9c17-f0af9ad08e4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "9cd3154e-073a-4942-b831-35dda034a58a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "a1a3173a-a425-4ef7-9320-3de5902b8d8e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/580b5f05-f66e-4cce-8060-7af8212ed30c")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4ab369db-39ef-4165-8b93-3cf4cd634668")
		)
		(fp_line
			(start 1.33 -1.27)
			(end 1.33 -6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "85a4e94b-8179-4008-9c2a-d7e3efebe321")
		)
		(fp_line
			(start 0 1.33)
			(end 1.33 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "548a1084-c2c7-40cb-9c9f-b54acd22d235")
		)
		(fp_line
			(start -1.33 -1.27)
			(end 1.33 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "88f048b4-ae49-4b06-b114-ea08380807e0")
		)
		(fp_line
			(start -1.33 -1.27)
			(end -1.33 -6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4a9ff970-0a90-4351-8c0b-efbac1319d28")
		)
		(fp_line
			(start -1.33 -6.41)
			(end 1.33 -6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3a486444-8c9f-448b-bab6-943bebd80491")
		)
		(fp_line
			(start 1.75 1.8)
			(end 1.75 -6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4617cd11-fd7f-4df5-ba89-fa1f7dc1dad2")
		)
		(fp_line
			(start 1.75 -6.85)
			(end -1.8 -6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "33100cce-e10a-4a12-b79d-91fafce2fe05")
		)
		(fp_line
			(start -1.8 1.8)
			(end 1.75 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9c3158df-f45d-4aac-a410-a700fdf79b93")
		)
		(fp_line
			(start -1.8 -6.85)
			(end -1.8 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2f9815f1-908a-4dce-b2ad-32cb1d605dcb")
		)
		(fp_line
			(start 1.27 0.635)
			(end 1.27 -6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "58240144-ae89-42b9-8ad8-6fc7cb3f7456")
		)
		(fp_line
			(start 1.27 -6.35)
			(end -1.27 -6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9c1d9e51-6148-4365-b961-06e9595cc0e2")
		)
		(fp_line
			(start 0.635 1.27)
			(end 1.27 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a6447814-02f4-47a1-a8ae-7f2ca2c97edc")
		)
		(fp_line
			(start -1.27 1.27)
			(end 0.635 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "36fa24b9-465e-4aa6-babd-959977333549")
		)
		(fp_line
			(start -1.27 -6.35)
			(end -1.27 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6a2a2386-c728-4585-8434-ef57d95761eb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.54 90)
			(layer "B.Fab")
			(uuid "a7f02e6a-6f1c-48ac-8330-8cef4a1e470e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "8cafaa0b-8e1b-4bb5-84d4-b416a2d267e3")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/RPM")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "d8e60554-ee5c-4826-9f29-6872ecab6eb1")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "1b42d74b-9a9a-495b-914a-f205f4f3a447")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "B.Cu")
		(uuid "f3a0eb19-f3b9-4e3e-9800-213b15b3be22")
		(at 220.847974 80.076673 90)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J9"
			(at 1 2.9 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "490133e5-5328-47dc-8e81-b3bd26aeeeba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "NTC"
			(at 1 -4 90)
			(layer "B.Fab")
			(uuid "805da15e-45f7-442e-b097-d9a1567d1757")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "c05f2715-103a-48fe-b0ba-e7b725ca1798")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "8f9710f1-e629-4c86-9a65-0012f745a9e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/e2d82743-21ff-464c-8ad7-c58cbb19ecd3")
		(sheetname "/")
		(sheetfile "scheda_banco_prova.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 3.45 -2.3)
			(end 3.45 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "67939399-a27f-46c3-b299-79b13192a52c")
		)
		(fp_line
			(start 1 -2.3)
			(end 1 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6b2e6952-5dc4-43d5-864e-aca266523385")
		)
		(fp_line
			(start 0.9 -2.3)
			(end 0.9 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c758541a-4260-486b-b414-56a314dcfff4")
		)
		(fp_line
			(start -1.45 -2.3)
			(end 3.45 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1dd4e501-6bad-4ce1-a488-e21ab239a75e")
		)
		(fp_line
			(start 1.1 -1.8)
			(end 1.1 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a366e7a0-b5d6-4d3a-8672-eb206a7c1264")
		)
		(fp_line
			(start 0.9 -1.8)
			(end 1.1 -1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "289cc77b-43b4-4f25-b8b7-bff8fa8415e2")
		)
		(fp_line
			(start 4.06 -0.8)
			(end 3.45 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3d3dde06-50a0-47a7-98ae-51f035761fe9")
		)
		(fp_line
			(start -2.06 -0.8)
			(end -1.45 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b90829a9-1bd0-4238-a692-4e64639385b7")
		)
		(fp_line
			(start 4.06 0.5)
			(end 3.45 0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bd603205-31ef-450a-95fb-4f58e266e46f")
		)
		(fp_line
			(start -2.06 0.5)
			(end -1.45 0.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "104f6959-3079-44c7-bc44-97134993c60a")
		)
		(fp_line
			(start 3.45 1.2)
			(end 1.5 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "db5770e6-b475-47f4-b952-51cea6c5f352")
		)
		(fp_line
			(start 1.5 1.2)
			(end 1.5 1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0c69cf98-0621-4283-b4cf-5a899d821f05")
		)
		(fp_line
			(start 0.5 1.2)
			(end -1.45 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "77306f22-0383-4040-ae20-28b06abadef1")
		)
		(fp_line
			(start -1.45 1.2)
			(end -1.45 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4e63117a-2193-4440-90b9-14ab094225ea")
		)
		(fp_line
			(start 0.5 1.81)
			(end 0.5 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "145dba4b-3789-4798-aaaa-35325b1d8047")
		)
		(fp_line
			(start -0.3 1.81)
			(end -0.3 2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d8c07f49-038a-43e3-bc3d-ffc26d730c34")
		)
		(fp_line
			(start -0.3 1.91)
			(end -0.6 1.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6b742d73-ffa3-4136-9e67-8a3d8b337c3a")
		)
		(fp_line
			(start -0.3 2.01)
			(end -0.6 2.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b0e0563d-f471-44de-97eb-e59cc0d85834")
		)
		(fp_line
			(start -0.6 2.01)
			(end -0.6 1.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c3933919-99b2-44da-82a8-040c3acba935")
		)
		(fp_line
			(start -1.11 2.11)
			(end -2.36 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dc734efb-9744-4327-a2d5-c9ae89b84590")
		)
		(fp_line
			(start -2.36 2.11)
			(end -2.36 0.86)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6310c8f3-e05e-4b0c-91fc-9a0479ddab91")
		)
		(fp_rect
			(start -2.06 1.81)
			(end 4.06 -2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "0c63dadf-a550-417a-ad7f-a33eb7581d2f")
		)
		(fp_rect
			(start -2.45 2.2)
			(end 4.45 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "90b263ae-b6f3-4015-aa7d-3c16a084bed7")
		)
		(fp_line
			(start -1.11 2.11)
			(end -2.36 2.11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "13e67366-2ab8-46cf-b007-2b34687308fa")
		)
		(fp_line
			(start -2.36 2.11)
			(end -2.36 0.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7a51d649-80c4-4815-a97f-91b728f6d1d2")
		)
		(fp_rect
			(start -1.95 1.7)
			(end 3.95 -2.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "b60deced-5b24-4848-9ffc-9749b7585f56")
		)
		(fp_text user "${REFERENCE}"
			(at 1 -1.5 90)
			(layer "B.Fab")
			(uuid "a54f2536-9ac2-4fae-9b04-dd46b02c2bd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 8 "/NTC_ADC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ab0b32af-aebd-44d7-bcd0-18681d55c5f3")
		)
		(pad "2" thru_hole oval
			(at 2 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "1fbc7ccb-71bd-4183-91cc-3dc217c56b90")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 134.95 93.5)
		(end 168.95 93.5)
		(stroke
			(width 0.16)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "4d39f37c-82b0-4297-991d-5e3f02ac3e50")
	)
	(gr_circle
		(center 134.95 93.5)
		(end 168.95 93.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "Margin")
		(uuid "dbb84c0f-8ac3-4c6b-b96a-1e774551e1f8")
	)
	(gr_circle
		(center 134.95 93.5)
		(end 164.55 93.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "User.1")
		(uuid "e034b71f-5026-4497-9544-dcf16c23f7bc")
	)
	(segment
		(start 77.9875 108)
		(end 76.75 108)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "f5c89aef-bf04-4769-b8f9-77af0700854f")
	)
	(via
		(at 76.75 108)
		(size 0.6)
		(drill 0.3)
		(layers "F.Cu" "B.Cu")
		(net 4)
		(uuid "358af99c-cbac-4e31-a80b-3d4591f9e384")
	)
	(segment
		(start 80.150001 111.299999)
		(end 79.950001 111.299999)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "1419ba61-54e3-4fb5-8716-5c2c8f0009b2")
	)
	(segment
		(start 78.0875 113.1625)
		(end 78.0875 113.2)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "448b41a7-6b2e-4625-9be4-7a4b24487092")
	)
	(segment
		(start 80.149999 109.400001)
		(end 80.149999 111.299997)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "5bb1c7ea-dcb1-444c-83d9-8acb284956d0")
	)
	(segment
		(start 79.950001 111.299999)
		(end 78.0875 113.1625)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "99c6acc1-d87f-46d8-b903-2148abb41edf")
	)
	(segment
		(start 80.149999 111.299997)
		(end 80.150001 111.299999)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "b046c54e-7006-4099-bd48-5ef7ffd37982")
	)
	(segment
		(start 75.7 108.9625)
		(end 75.712501 108.949999)
		(width 0.2)
		(layer "F.Cu")
		(net 14)
		(uuid "499dfd5d-212a-4df6-9269-505476e17283")
	)
	(segment
		(start 73.65 108.9625)
		(end 75.7 108.9625)
		(width 0.2)
		(layer "F.Cu")
		(net 14)
		(uuid "c97f9ccf-acb5-48ae-a51e-002c690d8115")
	)
	(segment
		(start 80.150001 107.399999)
		(end 80.150001 104.35)
		(width 0.2)
		(layer "F.Cu")
		(net 36)
		(uuid "1ba08dbc-9d09-4cba-9c7e-8b49486eb31c")
	)
	(segment
		(start 77.987499 104.562501)
		(end 78.250002 104.299998)
		(width 0.2)
		(layer "F.Cu")
		(net 36)
		(uuid "25d1d3d6-77b7-4780-9dbd-7889b26e3f2c")
	)
	(segment
		(start 78.250002 104.299998)
		(end 80.099999 104.299998)
		(width 0.2)
		(layer "F.Cu")
		(net 36)
		(uuid "624c660f-abdb-4ef9-a247-ce85f1870bcb")
	)
	(segment
		(start 77.987499 107.050001)
		(end 77.987499 104.562501)
		(width 0.2)
		(layer "F.Cu")
		(net 36)
		(uuid "bdebd0ff-a573-40ad-b288-ce428fde3740")
	)
	(segment
		(start 80.150001 104.35)
		(end 80.099999 104.299998)
		(width 0.2)
		(layer "F.Cu")
		(net 36)
		(uuid "e2cc9242-3eb6-4c87-b8d3-ff4c6d40d42b")
	)
	(segment
		(start 78.050001 109.012501)
		(end 77.9875 108.95)
		(width 0.2)
		(layer "F.Cu")
		(net 42)
		(uuid "29c62587-638f-4a7c-9d4e-ad94888f2b4f")
	)
	(segment
		(start 78.050001 110.800001)
		(end 78.050001 109.012501)
		(width 0.2)
		(layer "F.Cu")
		(net 42)
		(uuid "8f2aa7f8-5185-48b5-83ba-6a064ced7a88")
	)
	(segment
		(start 75.45 104.3)
		(end 74.000001 104.3)
		(width 0.2)
		(layer "F.Cu")
		(net 45)
		(uuid "0733eeb4-633d-4960-a2c9-c136c9f6d76b")
	)
	(segment
		(start 75.7125 104.5625)
		(end 75.45 104.3)
		(width 0.2)
		(layer "F.Cu")
		(net 45)
		(uuid "858ba8e7-d71a-49b4-a28d-d37146b46191")
	)
	(segment
		(start 75.7125 107.05)
		(end 75.7125 104.5625)
		(width 0.2)
		(layer "F.Cu")
		(net 45)
		(uuid "8ca20348-055e-4fca-b433-323a5bb66a43")
	)
	(zone
		(net 45)
		(net_name "/BOUT_P")
		(layer "F.Cu")
		(uuid "334700a2-251c-4a65-be9e-9ca3c0f4ab45")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 73.95 102.7) (xy 70.05 101.4) (xy 70.05 107.2) (xy 73.95 105.9)
			)
		)
	)
	(embedded_fonts no)
)
