(footprint "SOP65P490X110-8N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.175 -2.535 0)
		(layer "F.SilkS")
		(uuid "df14d031-892f-42e3-98fc-a44d846aa003")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SOP65P490X110-8N"
		(at 7.16 2.535 0)
		(layer "F.Fab")
		(uuid "912f3fc9-fa88-442a-8305-3281bf678b3c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e1f0ae39-11a3-4756-a7cf-5ec3fbae3569")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "38ecc4f8-26ec-4504-9884-7bcfc9ff8954")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.5 -1.535)
		(end 1.5 -1.535)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "566560d9-3d6f-48af-b03f-8747f66b2561")
	)
	(fp_line
		(start -1.5 1.535)
		(end 1.5 1.535)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7680e29e-5ec2-4031-b060-578b00da5b7e")
	)
	(fp_circle
		(center -3.52 -1.255)
		(end -3.42 -1.255)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "ed313a0f-74ef-4af6-b501-9624edadad9c")
	)
	(fp_line
		(start -3.135 -1.75)
		(end -3.135 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "21e7a3de-6e0c-49fd-83df-3b7b7ead4187")
	)
	(fp_line
		(start -3.135 -1.75)
		(end 3.135 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "21f5e5af-e16d-48fb-a37b-e538eecbbc4a")
	)
	(fp_line
		(start -3.135 1.75)
		(end 3.135 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d589418b-0cf5-4fad-b4bc-abec1c930c73")
	)
	(fp_line
		(start 3.135 -1.75)
		(end 3.135 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b676e545-08d0-4ad1-8b13-b6f0b69f2b5c")
	)
	(fp_line
		(start -1.5 -1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "98df643b-6722-488e-9d15-0bf2b828acce")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cd174b0b-0241-470b-b9e4-04d43fe5f26f")
	)
	(fp_line
		(start -1.5 1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8fc44fe7-974c-4c86-8763-8bca00592a1d")
	)
	(fp_line
		(start 1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "38df345d-6d3c-4a85-b46d-03162d49e6a3")
	)
	(fp_circle
		(center -3.52 -1.255)
		(end -3.42 -1.255)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5912b50b-b02e-48d2-8084-f76231f199c5")
	)
	(pad "1" smd roundrect
		(at -2.15 -0.975)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "9c9fc049-7876-424c-8aac-06fb7f5af081")
	)
	(pad "2" smd roundrect
		(at -2.15 -0.325)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "15b70f8f-340e-4340-ac32-4b8c8354997d")
	)
	(pad "3" smd roundrect
		(at -2.15 0.325)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "f5fe4134-a605-496a-9114-839b4107d58a")
	)
	(pad "4" smd roundrect
		(at -2.15 0.975)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "7f49dd1e-3942-4ffc-b39a-ba99e1b83d3c")
	)
	(pad "5" smd roundrect
		(at 2.15 0.975)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "b800b874-f4c0-45b9-9e36-479d8ff997e9")
	)
	(pad "6" smd roundrect
		(at 2.15 0.325)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "afc7c1ab-acbd-4581-b93a-21cf15f17914")
	)
	(pad "7" smd roundrect
		(at 2.15 -0.325)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "3f071ce2-a8a7-46f8-926d-ccadd92d49ac")
	)
	(pad "8" smd roundrect
		(at 2.15 -0.975)
		(size 1.47 0.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(solder_mask_margin 0.102)
		(uuid "c1ea3743-6d33-4f53-ba8e-03d02aecd607")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/footprints/Regulators.pretty/LM74610QDGKRQ1.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
