
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "NEO-M9N-00B" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -22.86 28.702 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "NEO-M9N-00B" (id 1) (at -22.86 -30.48 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "NEO-M9N-00B:XCVR_NEO-M9N-00B" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "DigiKey_Part_Number" "672-NEO-M9N-00BCT-ND" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/NEO-M9N-00B/u-blox/view-part/?ref=snap" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "2.6mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "SMD-24 u-blox" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/NEO-M9N-00B/u-blox/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "R05" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "u-blox" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "NEO-M9N-00B" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            series RF Receiver BeiDou, Galileo, GLONASS, GNSS, GPS - -167dBm - - Module\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "U blox" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "NEO-M9N-00B_0_0"
      (rectangle (start -22.86 -27.94) (end 22.86 27.94)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin output line (at 27.94 -2.54 180.0) (length 5.08)
        (name "LNA_EN"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at 27.94 -20.32 180.0) (length 5.08)
        (name "RESERVED"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at 27.94 -20.32 180.0) (length 5.08)
        (name "RESERVED"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at 27.94 -20.32 180.0) (length 5.08)
        (name "RESERVED"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -27.94 -12.7 0) (length 5.08)
        (name "SDA/SPI_CS_N"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional clock (at -27.94 -10.16 0) (length 5.08)
        (name "SCL/SPI_CLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at -27.94 -2.54 0) (length 5.08)
        (name "TXD/SPI_MISO"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 -5.08 0) (length 5.08)
        (name "RXD/SPI_MOSI"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 20.32 180.0) (length 5.08)
        (name "V_BCKP"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 25.4 180.0) (length 5.08)
        (name "VCC"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -25.4 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -25.4 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -25.4 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 -25.4 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 12.7 0) (length 5.08)
        (name "RF_IN"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 17.78 180.0) (length 5.08)
        (name "VCC_RF"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 15.24 0) (length 5.08)
        (name "RESET_N"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 27.94 22.86 180.0) (length 5.08)
        (name "V_USB"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -27.94 -20.32 0) (length 5.08)
        (name "USB_DP"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -27.94 -17.78 0) (length 5.08)
        (name "USB_DM"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 2.54 0) (length 5.08)
        (name "EXTINT"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 27.94 2.54 180.0) (length 5.08)
        (name "TIMEPULSE"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 5.08 0) (length 5.08)
        (name "D_SEL"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -27.94 7.62 0) (length 5.08)
        (name "SAFEBOOT_N"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)