(footprint "VG039NCHXTB222" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0.1 -2.4 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp d7dbcfe6-b89e-42a3-87cc-c16c0489151f)
  )
  (fp_text value "VG039NCHXTB222" (at 0.009861 5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 17c40e10-896f-4713-8e03-a9c368dc1840)
  )
  (fp_text user "${REFERENCE}" (at 0.009861 6.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 29945389-3afb-4dd0-99dd-08256f7b6768)
  )
  (fp_line (start -1.55 -0.1) (end -0.85 -0.1)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 70ced55b-09c8-466e-94bf-0ac1cce271fe))
  (fp_line (start -1.55 2.5) (end -1.55 -0.1)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 91f28639-e509-4ee3-ada5-d06102609c91))
  (fp_line (start -0.25 3.15) (end 0.35 3.15)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 24bdb3be-682c-4886-97f8-445833457c01))
  (fp_line (start 1.65 -0.05) (end 0.95 -0.05)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp bcdbc567-8649-4889-812b-4912dc893ad1))
  (fp_line (start 1.65 2.5) (end 1.65 -0.05)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 8b686eda-1441-4723-a931-a21b8e7845a4))
  (fp_circle (center -1.9 3.7) (end -1.719722 3.7)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e0f40886-c12d-4ad4-aca4-75f6bcc64fd5))
  (fp_circle (center 0.05 1.6) (end -0.45 1.15)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 1ebb7a0e-ebcb-4828-9de8-972f94075949))
  (pad "1" smd roundrect (at -0.95 3.45) (size 1.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 9faaeda2-09f4-49cc-a5ca-8b2100c46b42))
  (pad "2" smd roundrect (at 0.05 -0.25) (size 1.6 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 46355834-9626-4f43-b5f7-0a7edfcedd48))
  (pad "3" smd roundrect (at 1.05 3.45) (size 1.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 2e7b50f3-987a-4c84-9535-6cbfe6b4184d))
  (group "" (id 060f96bd-c3b8-48b6-9706-70fe80d68183)
    (members
      1ebb7a0e-ebcb-4828-9de8-972f94075949
      24bdb3be-682c-4886-97f8-445833457c01
      70ced55b-09c8-466e-94bf-0ac1cce271fe
      8b686eda-1441-4723-a931-a21b8e7845a4
      91f28639-e509-4ee3-ada5-d06102609c91
      bcdbc567-8649-4889-812b-4912dc893ad1
    )
  )
)
