(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CH32V003AxMx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V003AxMx"
			(at 7.62 15.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:STC_SOP-16_3.9x9.9mm_P1.27mm"
			(at -2.54 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at -2.54 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU microcontroller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*SO*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V003AxMx_1_1"
			(rectangle
				(start -7.62 12.7)
				(end 7.62 -12.7)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS_1" bidirectional line)
				(alternate "T1CH3_1" bidirectional line)
				(alternate "T2CH3" bidirectional line)
				(alternate "T2CH3_2" bidirectional line)
				(alternate "UTX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS" bidirectional line)
				(alternate "SDA" bidirectional line)
				(alternate "T1BKIN_1" bidirectional line)
				(alternate "T1BKIN_3" bidirectional line)
				(alternate "T2CH1ETR_2" bidirectional line)
				(alternate "T2CH1ETR_3" bidirectional line)
				(alternate "T2CH4_1" bidirectional line)
				(alternate "URX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR_1" bidirectional line)
				(alternate "SCL" bidirectional line)
				(alternate "T1BKIN" bidirectional line)
				(alternate "T1BKIN_2" bidirectional line)
				(alternate "T1ETR_3" bidirectional line)
				(alternate "T2CH2_1" bidirectional line)
				(alternate "URTS" bidirectional line)
				(alternate "URTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "T1CH1N_1" bidirectional line)
				(alternate "T1CH1N_3" bidirectional line)
				(alternate "T1CH3" bidirectional line)
				(alternate "T1CH3_2" bidirectional line)
				(alternate "UCTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A2" bidirectional line)
				(alternate "MCO" bidirectional line)
				(alternate "T1CH1_3" bidirectional line)
				(alternate "T1CH2N_1" bidirectional line)
				(alternate "T1CH4" bidirectional line)
				(alternate "T1CH4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MOSI" bidirectional line)
				(alternate "MOSI_1" bidirectional line)
				(alternate "SDA_2" bidirectional line)
				(alternate "SDA_3" bidirectional line)
				(alternate "T1CH1_1" bidirectional line)
				(alternate "T1CH3N_3" bidirectional line)
				(alternate "UCTS_2" bidirectional line)
				(alternate "UCTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MISO" bidirectional line)
				(alternate "MISO_1" bidirectional line)
				(alternate "T1CH2_1" bidirectional line)
				(alternate "T1CH2_3" bidirectional line)
				(alternate "T2CH2_3" bidirectional line)
				(alternate "URTS_2" bidirectional line)
				(alternate "URTS_3" bidirectional line)
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR2" bidirectional line)
				(alternate "SCL_1" bidirectional line)
				(alternate "SWIO" bidirectional line)
				(alternate "T1CH3N" bidirectional line)
				(alternate "T1CH3N_1" bidirectional line)
				(alternate "T1CH3N_2" bidirectional line)
				(alternate "URX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A7" bidirectional line)
				(alternate "OPO" bidirectional line)
				(alternate "T1CH4_3" bidirectional line)
				(alternate "T2CH1ETR" bidirectional line)
				(alternate "TIETR_2" bidirectional line)
				(alternate "UCK" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A5" bidirectional line)
				(alternate "T2CH4_3" bidirectional line)
				(alternate "URX_2" bidirectional line)
				(alternate "UTX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A6" bidirectional line)
				(alternate "T2CH3_3" bidirectional line)
				(alternate "URX" bidirectional line)
				(alternate "UTX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NRST" bidirectional line)
				(alternate "OPP1" bidirectional line)
				(alternate "T2CH4" bidirectional line)
				(alternate "T2CH4_2" bidirectional line)
				(alternate "UCK_1" bidirectional line)
				(alternate "UCK_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A1" bidirectional line)
				(alternate "OPN0" bidirectional line)
				(alternate "OSCI" bidirectional line)
				(alternate "T1CH2" bidirectional line)
				(alternate "T1CH2_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A0" bidirectional line)
				(alternate "AETR2_1" bidirectional line)
				(alternate "OPP0" bidirectional line)
				(alternate "OSCO" bidirectional line)
				(alternate "TICH2N" bidirectional line)
				(alternate "TICH2N_2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V003FxPx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V003FxPx"
			(at 7.62 17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -1.27 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at -1.27 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "microcontroller wch RISC-V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V003FxPx_1_1"
			(rectangle
				(start -7.62 15.24)
				(end 7.62 -15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS_1" bidirectional line)
				(alternate "T1CH3_1" bidirectional line)
				(alternate "T2CH3" bidirectional line)
				(alternate "T2CH3_2" bidirectional line)
				(alternate "UTX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS" bidirectional line)
				(alternate "SDA" bidirectional line)
				(alternate "T1BKIN_1" bidirectional line)
				(alternate "T1BKIN_3" bidirectional line)
				(alternate "T2CH1ETR_2" bidirectional line)
				(alternate "T2CH1ETR_3" bidirectional line)
				(alternate "T2CH4_1" bidirectional line)
				(alternate "URX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR_1" bidirectional line)
				(alternate "SCL" bidirectional line)
				(alternate "T1BKIN" bidirectional line)
				(alternate "T1BKIN_2" bidirectional line)
				(alternate "T1ETR_3" bidirectional line)
				(alternate "T2CH2_1" bidirectional line)
				(alternate "URTS" bidirectional line)
				(alternate "URTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "T1CH1N_1" bidirectional line)
				(alternate "T1CH1N_3" bidirectional line)
				(alternate "T1CH3" bidirectional line)
				(alternate "T1CH3_2" bidirectional line)
				(alternate "UCTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A2" bidirectional line)
				(alternate "MCO" bidirectional line)
				(alternate "T1CH1_3" bidirectional line)
				(alternate "T1CH2N_1" bidirectional line)
				(alternate "T1CH4" bidirectional line)
				(alternate "T1CH4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SCK" bidirectional line)
				(alternate "SCK_1" bidirectional line)
				(alternate "SCL_2" bidirectional line)
				(alternate "SCL_3" bidirectional line)
				(alternate "T1CH3_3" bidirectional line)
				(alternate "T1ETR" bidirectional line)
				(alternate "T1ETR_1" bidirectional line)
				(alternate "T2CH1ETR_1" bidirectional line)
				(alternate "UCK_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MOSI" bidirectional line)
				(alternate "MOSI_1" bidirectional line)
				(alternate "SDA_2" bidirectional line)
				(alternate "SDA_3" bidirectional line)
				(alternate "T1CH1_1" bidirectional line)
				(alternate "T1CH3N_3" bidirectional line)
				(alternate "UCTS_2" bidirectional line)
				(alternate "UCTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MISO" bidirectional line)
				(alternate "MISO_1" bidirectional line)
				(alternate "T1CH2_1" bidirectional line)
				(alternate "T1CH2_3" bidirectional line)
				(alternate "T2CH2_3" bidirectional line)
				(alternate "URTS_2" bidirectional line)
				(alternate "URTS_3" bidirectional line)
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPN1" bidirectional line)
				(alternate "SDA_1" bidirectional line)
				(alternate "TICH1N" bidirectional line)
				(alternate "TICH1N_2" bidirectional line)
				(alternate "UTX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR2" bidirectional line)
				(alternate "SCL_1" bidirectional line)
				(alternate "SWIO" bidirectional line)
				(alternate "T1CH3N" bidirectional line)
				(alternate "T1CH3N_1" bidirectional line)
				(alternate "T1CH3N_2" bidirectional line)
				(alternate "URX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A3" bidirectional line)
				(alternate "T1CH1" bidirectional line)
				(alternate "T1CH1_2" bidirectional line)
				(alternate "T1CH2N_3" bidirectional line)
				(alternate "T2CH3_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A4" bidirectional line)
				(alternate "AETR" bidirectional line)
				(alternate "T1CH4_1" bidirectional line)
				(alternate "T2CH2" bidirectional line)
				(alternate "T2CH2_2" bidirectional line)
				(alternate "UCTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A7" bidirectional line)
				(alternate "OPO" bidirectional line)
				(alternate "T1CH4_3" bidirectional line)
				(alternate "T2CH1ETR" bidirectional line)
				(alternate "TIETR_2" bidirectional line)
				(alternate "UCK" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A5" bidirectional line)
				(alternate "T2CH4_3" bidirectional line)
				(alternate "URX_2" bidirectional line)
				(alternate "UTX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A6" bidirectional line)
				(alternate "T2CH3_3" bidirectional line)
				(alternate "URX" bidirectional line)
				(alternate "UTX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NRST" bidirectional line)
				(alternate "OPP1" bidirectional line)
				(alternate "T2CH4" bidirectional line)
				(alternate "T2CH4_2" bidirectional line)
				(alternate "UCK_1" bidirectional line)
				(alternate "UCK_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A1" bidirectional line)
				(alternate "OPN0" bidirectional line)
				(alternate "OSCI" bidirectional line)
				(alternate "T1CH2" bidirectional line)
				(alternate "T1CH2_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A0" bidirectional line)
				(alternate "AETR2_1" bidirectional line)
				(alternate "OPP0" bidirectional line)
				(alternate "OSCO" bidirectional line)
				(alternate "TICH2N" bidirectional line)
				(alternate "TICH2N_2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V003FxUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V003FxUx"
			(at 7.62 17.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at -1.27 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at -1.27 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "microcontroller wch RISC-V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.4mm*EP1.65x1.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V003FxUx_1_1"
			(rectangle
				(start -7.62 15.24)
				(end 7.62 -15.24)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS_1" bidirectional line)
				(alternate "T1CH3_1" bidirectional line)
				(alternate "T2CH3" bidirectional line)
				(alternate "T2CH3_2" bidirectional line)
				(alternate "UTX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS" bidirectional line)
				(alternate "SDA" bidirectional line)
				(alternate "T1BKIN_1" bidirectional line)
				(alternate "T1BKIN_3" bidirectional line)
				(alternate "T2CH1ETR_2" bidirectional line)
				(alternate "T2CH1ETR_3" bidirectional line)
				(alternate "T2CH4_1" bidirectional line)
				(alternate "URX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR_1" bidirectional line)
				(alternate "SCL" bidirectional line)
				(alternate "T1BKIN" bidirectional line)
				(alternate "T1BKIN_2" bidirectional line)
				(alternate "T1ETR_3" bidirectional line)
				(alternate "T2CH2_1" bidirectional line)
				(alternate "URTS" bidirectional line)
				(alternate "URTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "T1CH1N_1" bidirectional line)
				(alternate "T1CH1N_3" bidirectional line)
				(alternate "T1CH3" bidirectional line)
				(alternate "T1CH3_2" bidirectional line)
				(alternate "UCTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A2" bidirectional line)
				(alternate "MCO" bidirectional line)
				(alternate "T1CH1_3" bidirectional line)
				(alternate "T1CH2N_1" bidirectional line)
				(alternate "T1CH4" bidirectional line)
				(alternate "T1CH4_2" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SCK" bidirectional line)
				(alternate "SCK_1" bidirectional line)
				(alternate "SCL_2" bidirectional line)
				(alternate "SCL_3" bidirectional line)
				(alternate "T1CH3_3" bidirectional line)
				(alternate "T1ETR" bidirectional line)
				(alternate "T1ETR_1" bidirectional line)
				(alternate "T2CH1ETR_1" bidirectional line)
				(alternate "UCK_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MOSI" bidirectional line)
				(alternate "MOSI_1" bidirectional line)
				(alternate "SDA_2" bidirectional line)
				(alternate "SDA_3" bidirectional line)
				(alternate "T1CH1_1" bidirectional line)
				(alternate "T1CH3N_3" bidirectional line)
				(alternate "UCTS_2" bidirectional line)
				(alternate "UCTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MISO" bidirectional line)
				(alternate "MISO_1" bidirectional line)
				(alternate "T1CH2_1" bidirectional line)
				(alternate "T1CH2_3" bidirectional line)
				(alternate "T2CH2_3" bidirectional line)
				(alternate "URTS_2" bidirectional line)
				(alternate "URTS_3" bidirectional line)
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPN1" bidirectional line)
				(alternate "SDA_1" bidirectional line)
				(alternate "TICH1N" bidirectional line)
				(alternate "TICH1N_2" bidirectional line)
				(alternate "UTX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR2" bidirectional line)
				(alternate "SCL_1" bidirectional line)
				(alternate "SWIO" bidirectional line)
				(alternate "T1CH3N" bidirectional line)
				(alternate "T1CH3N_1" bidirectional line)
				(alternate "T1CH3N_2" bidirectional line)
				(alternate "URX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A3" bidirectional line)
				(alternate "T1CH1" bidirectional line)
				(alternate "T1CH1_2" bidirectional line)
				(alternate "T1CH2N_3" bidirectional line)
				(alternate "T2CH3_1" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A4" bidirectional line)
				(alternate "AETR" bidirectional line)
				(alternate "T1CH4_1" bidirectional line)
				(alternate "T2CH2" bidirectional line)
				(alternate "T2CH2_2" bidirectional line)
				(alternate "UCTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A7" bidirectional line)
				(alternate "OPO" bidirectional line)
				(alternate "T1CH4_3" bidirectional line)
				(alternate "T2CH1ETR" bidirectional line)
				(alternate "TIETR_2" bidirectional line)
				(alternate "UCK" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A5" bidirectional line)
				(alternate "T2CH4_3" bidirectional line)
				(alternate "URX_2" bidirectional line)
				(alternate "UTX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A6" bidirectional line)
				(alternate "T2CH3_3" bidirectional line)
				(alternate "URX" bidirectional line)
				(alternate "UTX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NRST" bidirectional line)
				(alternate "OPP1" bidirectional line)
				(alternate "T2CH4" bidirectional line)
				(alternate "T2CH4_2" bidirectional line)
				(alternate "UCK_1" bidirectional line)
				(alternate "UCK_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A1" bidirectional line)
				(alternate "OPN0" bidirectional line)
				(alternate "OSCI" bidirectional line)
				(alternate "T1CH2" bidirectional line)
				(alternate "T1CH2_2" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A0" bidirectional line)
				(alternate "AETR2_1" bidirectional line)
				(alternate "OPP0" bidirectional line)
				(alternate "OSCO" bidirectional line)
				(alternate "TICH2N" bidirectional line)
				(alternate "TICH2N_2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V003JxMx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V003JxMx"
			(at 15.24 7.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:JEITA_SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios. JEITA SOIC-8 (SOP-8)"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "microcontroller wch RISC-V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "JEITA?SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V003JxMx_1_1"
			(rectangle
				(start -15.24 5.08)
				(end 15.24 -5.08)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "NSS" bidirectional line)
				(alternate "SDA" bidirectional line)
				(alternate "T1BKIN_1" bidirectional line)
				(alternate "T1BKIN_3" bidirectional line)
				(alternate "T2CH1ETR_2" bidirectional line)
				(alternate "T2CH1ETR_3" bidirectional line)
				(alternate "T2CH4_1" bidirectional line)
				(alternate "URX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AETR_1" bidirectional line)
				(alternate "SCL" bidirectional line)
				(alternate "T1BKIN" bidirectional line)
				(alternate "T1BKIN_2" bidirectional line)
				(alternate "T1ETR_3" bidirectional line)
				(alternate "T2CH2_1" bidirectional line)
				(alternate "URTS" bidirectional line)
				(alternate "URTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A2" bidirectional line)
				(alternate "MCO" bidirectional line)
				(alternate "T1CH1_3" bidirectional line)
				(alternate "T1CH2N_1" bidirectional line)
				(alternate "T1CH4" bidirectional line)
				(alternate "T1CH4_2" bidirectional line)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD1/PD4/PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A5" bidirectional line)
				(alternate "A7" bidirectional line)
				(alternate "AETR2" bidirectional line)
				(alternate "OPO" bidirectional line)
				(alternate "SCL_1" bidirectional line)
				(alternate "SWIO" bidirectional line)
				(alternate "T1CH3N" bidirectional line)
				(alternate "T1CH3N_1" bidirectional line)
				(alternate "T1CH3N_2" bidirectional line)
				(alternate "T1CH4_3" bidirectional line)
				(alternate "T2CH1ETR" bidirectional line)
				(alternate "T2CH4_3" bidirectional line)
				(alternate "TIETR_2" bidirectional line)
				(alternate "UCK" bidirectional line)
				(alternate "URX_1" bidirectional line)
				(alternate "URX_2" bidirectional line)
				(alternate "UTX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PD6/PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A1" bidirectional line)
				(alternate "A6" bidirectional line)
				(alternate "OPN0" bidirectional line)
				(alternate "OSCI" bidirectional line)
				(alternate "T1CH2" bidirectional line)
				(alternate "T1CH2_2" bidirectional line)
				(alternate "T2CH3_3" bidirectional line)
				(alternate "URX" bidirectional line)
				(alternate "UTX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "A0" bidirectional line)
				(alternate "AETR2_1" bidirectional line)
				(alternate "OPP0" bidirectional line)
				(alternate "OSCO" bidirectional line)
				(alternate "TICH2N" bidirectional line)
				(alternate "TICH2N_2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V005D6U6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.192 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V005D6U6"
			(at 9.652 12.192 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-12-1EP_2x2mm_P0.4mm_EP1.1x1.1mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH32V006DS0_PDF.html"
			(at 0 -30.734 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "QingKe 32-bit RISC-V core, 48MHz, 32KB Flash, 6KB RAM, 11 GPIO, UQFN-12"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "WCH WinChipHead Nanjing-Qinheng-Microelectronics ADC I2C SPI USART microcontroller MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*UQFN*2x2mm?P0.4mm?EP1.1*x1.1*mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V005D6U6_0_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V005D6U6_1_0"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI_MOSI_3" bidirectional line)
				(alternate "SPI_NSS_1" bidirectional line)
				(alternate "TIM1_CH1N_7" bidirectional line)
				(alternate "TIM1_CH1N_9" bidirectional line)
				(alternate "TIM1_CH3_2" bidirectional line)
				(alternate "TIM2_CH1_ETR_4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM1_CH1N_2" bidirectional line)
				(alternate "TIM1_CH1N_3" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "TIM1_CH3_5" bidirectional line)
				(alternate "TIM2_CH3_4" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" input line)
				(alternate "MCO" bidirectional line)
				(alternate "SPI_NSS_2" bidirectional line)
				(alternate "SPI_NSS_6" bidirectional line)
				(alternate "TIM1_CH1_3" bidirectional line)
				(alternate "TIM1_CH1_7" bidirectional line)
				(alternate "TIM1_CH1_8" bidirectional line)
				(alternate "TIM1_CH2N_2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_RX_9" bidirectional line)
				(alternate "USART2_TX_5" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C_SDA_2" bidirectional line)
				(alternate "SPI_MOSI" bidirectional line)
				(alternate "SPI_MOSI_1" bidirectional line)
				(alternate "TIM1_CH1_2" bidirectional line)
				(alternate "TIM1_CH3N_3" bidirectional line)
				(alternate "TIM1_CH3_7" bidirectional line)
				(alternate "TIM1_CH3_8" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
				(alternate "USART1_RX_6" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI_MISO" bidirectional line)
				(alternate "SPI_MISO_1" bidirectional line)
				(alternate "SPI_MISO_6" bidirectional line)
				(alternate "TIM1_CH2_2" bidirectional line)
				(alternate "TIM1_CH2_3" bidirectional line)
				(alternate "TIM1_CH4_7" bidirectional line)
				(alternate "TIM1_CH4_8" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
				(alternate "USART1_CTS_6" bidirectional line)
				(alternate "USART1_CTS_7" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C_SDA_1" bidirectional line)
				(alternate "OPA_N1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM1_CH3N_4" bidirectional line)
				(alternate "TIM1_CH3N_5" bidirectional line)
				(alternate "TIM1_CH3N_6" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IETR" bidirectional line)
				(alternate "I2C_SCL_1" bidirectional line)
				(alternate "I2C_SDA_4" bidirectional line)
				(alternate "OPA_P3" bidirectional line)
				(alternate "SWDIO" bidirectional line)
				(alternate "SWIO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM1_CH3N_2" bidirectional line)
				(alternate "TIM1_CH4_4" bidirectional line)
				(alternate "TIM1_CH4_5" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
				(alternate "USART1_RX_5" bidirectional line)
				(alternate "USART1_TX_4" bidirectional line)
				(alternate "USART2_RX_5" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "OPA_OUT0" bidirectional line)
				(alternate "SPI_SCK_4" bidirectional line)
				(alternate "TIM1_CH4_3" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "TIM1_ETR_4" bidirectional line)
				(alternate "TIM1_ETR_5" bidirectional line)
				(alternate "TIM1_ETR_6" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH2_7" bidirectional line)
				(alternate "USART1_RTS_9" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA_P1" bidirectional line)
				(alternate "RST" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "USART1_CTS_4" bidirectional line)
				(alternate "USART1_CTS_5" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "OPA_N0" bidirectional line)
				(alternate "SPI_SCK_5" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "TIM1_CH2_9" bidirectional line)
				(alternate "TIM2_CH2_5" bidirectional line)
				(alternate "TIM2_CH2_6" bidirectional line)
				(alternate "USART1_RX_8" bidirectional line)
				(alternate "USART2_RTS_2" bidirectional line)
				(alternate "USART2_RTS_3" bidirectional line)
				(alternate "USART2_RTS_4" bidirectional line)
				(alternate "USART2_RTS_5" bidirectional line)
				(alternate "XI" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IETR_1" bidirectional line)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "OPA_P0" bidirectional line)
				(alternate "SPI_MOSI_5" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM1_CH2N_4" bidirectional line)
				(alternate "TIM1_CH2N_5" bidirectional line)
				(alternate "TIM1_CH2N_6" bidirectional line)
				(alternate "TIM1_CH3_9" bidirectional line)
				(alternate "TIM2_CH3_5" bidirectional line)
				(alternate "TIM2_CH3_6" bidirectional line)
				(alternate "TIM2_CH3_7" bidirectional line)
				(alternate "USART2_TX_2" bidirectional line)
				(alternate "XO" bidirectional line)
			)
		)
		(symbol "CH32V005D6U6_1_1"
			(rectangle
				(start -10.16 10.16)
				(end 10.16 -10.16)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V203CxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V203CxTx"
			(at 6.858 38.862 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V203.html"
			(at 1.27 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V203 is an industrial-grade enhanced low-power general-purpose MCU based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V203CxTx_0_0"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD_VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V203CxTx_0_1"
			(rectangle
				(start -12.7 -38.1)
				(end 15.24 35.56)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "CH32V203CxTx_1_0"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TAMPER-RTC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN8" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" bidirectional line)
				(alternate "OPA1_OUT1" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "BOOT1" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_SCK_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "SPI1_MOSI_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "USART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX_2" bidirectional line)
				(alternate "I2C1_SCL_1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX_2" bidirectional line)
				(alternate "I2C1_SDA_1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN3" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" bidirectional line)
				(alternate "OPA2_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART4_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART4_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
				(alternate "USBDM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
				(alternate "USBDP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM2_CH13" bidirectional line)
				(alternate "TIM2_CH1_1" bidirectional line)
				(alternate "TIM2_ETR_1" bidirectional line)
				(alternate "TIM2_ETR_3" bidirectional line)
				(alternate "USART4_RTS_1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V203F6P6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V203F6P6"
			(at 2.54 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V203.html"
			(at 0 -6.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V203 is an industrial-grade enhanced low-power general-purpose MCU based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V203F6P6_0_1"
			(rectangle
				(start -10.16 -17.78)
				(end 10.16 17.78)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "CH32V203F6P6_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX_2" bidirectional line)
				(alternate "I2C1_SCL_1" bidirectional line)
				(alternate "PB8" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" input line)
				(alternate "OPA1_OUT1" output line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" output line)
				(alternate "TIM3_CH4_2" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "TIM2_CH1" passive line)
				(alternate "TIM2_CH1_2" bidirectional line)
				(alternate "TIM2_ETR" passive line)
				(alternate "TIM2_ETR_2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" input line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" passive line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" input line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "USART2_TX" output line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN3" input line)
				(alternate "OPA1_OUT0" output line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "USART2_RX" input line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" input line)
				(alternate "OPA2_OUT1" output line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" input line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" input line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" input line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" output line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" input line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" input line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" input line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
				(alternate "USBDM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" output line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
				(alternate "USBDP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V203GxUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 24.384 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32V203GxUx"
			(at 15.748 24.13 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-28-1EP_4x4mm_P0.4mm_EP2.7x2.7mm"
			(at -33.02 -21.59 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH32V203DS0_PDF.html"
			(at 0 37.084 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "NanjingQinheng WCH RISC-V MCU, 32-64KB flash, 10-20KB RAM, 144 MHz, 2.4-3.6V, 24 GPIO, ADC, OpAmp, CAN, USB, WQFN-28"
			(at -0.508 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISCV WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.4mm*EP2.7x2.7*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V203GxUx_1_1"
			(rectangle
				(start -22.86 22.86)
				(end 22.86 -20.32)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PA10/PA11/USB_D-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PA12/USB_D+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PA13/SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PA14/SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "BOOT0/PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "OSC_IN/PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "OSC_OUT/PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xCxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V30xCxTx"
			(at 5.08 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V30xCxTx_0_0"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V30xCxTx_1_0"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN3" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
				(alternate "USART7_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN8" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
		)
		(symbol "CH32V30xCxTx_1_1"
			(rectangle
				(start -12.7 35.56)
				(end 12.7 -35.56)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xFxPx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V30xFxPx"
			(at 2.54 20.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V30xFxPx_1_1"
			(rectangle
				(start -10.16 17.78)
				(end 10.16 -17.78)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA1/PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PA8/PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA9/PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
				(alternate "USART8_TX_1" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VIO" power_in line)
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xRxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V30xRxTx"
			(at 7.62 55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 0 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V30xRxTx_0_0"
			(pin power_in line
				(at -2.54 55.88 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 2.54)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V30xRxTx_1_0"
			(pin input line
				(at -15.24 45.72 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GTXC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN3" bidirectional line)
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MIS" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART7_TX_1" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DVP_D6" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -48.26 0)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at 0 55.88 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 55.88 270)
				(length 2.54)
				(hide yes)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
		)
		(symbol "CH32V30xRxTx_1_1"
			(rectangle
				(start -12.7 53.34)
				(end 12.7 -53.34)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xVxTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V30xVxTx"
			(at 5.08 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V30xVxTx_0_0"
			(pin bidirectional line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -55.88 0)
				(length 2.54)
				(name "VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -63.5 0)
				(length 2.54)
				(name "VREF-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V30xVxTx_1_0"
			(pin input line
				(at -17.78 63.5 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 60.96 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at -17.78 58.42 0)
				(length 2.54)
				(hide yes)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GTXC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "DVP_HSYNC" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "DVP_VSYNC" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" bidirectional line)
				(alternate "DVP_PCLK" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART7_TX_1" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART7_RX_1" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D0" bidirectional line)
				(alternate "OTG_FS_VBUS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH2_1" bidirectional line)
				(alternate "USART1_RTS_2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D1" bidirectional line)
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D5" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "DVP_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NADV" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "DVP_D6" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "DVP_D7" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at -2.54 71.12 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 71.12 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 63.5 180)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 60.96 180)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 58.42 180)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 55.88 180)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D2" bidirectional line)
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D3" bidirectional line)
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PC10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PC11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D4" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PC12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D9" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "FSMC_D2" bidirectional line)
				(alternate "TIM10_ETR_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "FSMC_D3" bidirectional line)
				(alternate "TIM10_CH1_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D11" bidirectional line)
				(alternate "FSMC_NADV" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "TIM10_CH2_2" bidirectional line)
				(alternate "USART2_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "USART2_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIM10_CH3_2" bidirectional line)
				(alternate "USART2_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DVP_D10" bidirectional line)
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "USART2_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NCE2" bidirectional line)
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM10_CH4_2" bidirectional line)
				(alternate "USART2_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "FSMC_D13" bidirectional line)
				(alternate "TIM9_CH1N_2" bidirectional line)
				(alternate "USART3_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PD9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "TIM9_CH1_ETR_2" bidirectional line)
				(alternate "USART3_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PD10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RMII_RXD1" bidirectional line)
				(alternate "FSMC_D15" bidirectional line)
				(alternate "TIM9-CH2N_2" bidirectional line)
				(alternate "USART3_CK_2" bidirectional line)
				(alternate "USART3_CK_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "TIM9_CH2_2" bidirectional line)
				(alternate "USART3_CTS_2" bidirectional line)
				(alternate "USART3_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "TIM9_CH3N_2" bidirectional line)
				(alternate "USART3_RTS_2" bidirectional line)
				(alternate "USART3_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2_1" bidirectional line)
				(alternate "TIM9_CH3_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D0" bidirectional line)
				(alternate "TIM4_CH3_1" bidirectional line)
				(alternate "TIM9_BKIN_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "TIM4_CH4_1" bidirectional line)
				(alternate "TIM9_CH4_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PE0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM4_ETR_1" bidirectional line)
				(alternate "UART4_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PE1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "UART4_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PE2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A23" bidirectional line)
				(alternate "TIM10_BKIN_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PE3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A19" bidirectional line)
				(alternate "TIM10_CH1N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PE4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A20" bidirectional line)
				(alternate "TIM10_CH2N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PE5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A21" bidirectional line)
				(alternate "TIM10_CH3N_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PE6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PE7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "OPA3_OUT1" bidirectional line)
				(alternate "TIM1_ETR_3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -45.72 180)
				(length 2.54)
				(name "PE8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "OPA4_OUT1" bidirectional line)
				(alternate "TIM1_CH1N_3" bidirectional line)
				(alternate "UART5_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -48.26 180)
				(length 2.54)
				(name "PE9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "TIM1_CH1_3" bidirectional line)
				(alternate "UART5_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -50.8 180)
				(length 2.54)
				(name "PE10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "TIM1_CH2N_3" bidirectional line)
				(alternate "UART6_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -53.34 180)
				(length 2.54)
				(name "PE11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "TIM1_CH2_3" bidirectional line)
				(alternate "UART6_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -55.88 180)
				(length 2.54)
				(name "PE12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D9" bidirectional line)
				(alternate "TIM1_CH3N_3" bidirectional line)
				(alternate "UART7_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -58.42 180)
				(length 2.54)
				(name "PE13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D10" bidirectional line)
				(alternate "TIM1_CH3_3" bidirectional line)
				(alternate "UART7_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -60.96 180)
				(length 2.54)
				(name "PE14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D11" bidirectional line)
				(alternate "OPA2_OUT1" bidirectional line)
				(alternate "TIM1_CH4_3" bidirectional line)
				(alternate "UART8_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -63.5 180)
				(length 2.54)
				(name "PE15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "OPA1_OUT1" bidirectional line)
				(alternate "TXM1_BKIN_3" bidirectional line)
				(alternate "UART8_RX_2" bidirectional line)
			)
		)
		(symbol "CH32V30xVxTx_1_1"
			(rectangle
				(start -15.24 68.58)
				(end 15.24 -68.58)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32V30xWxUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CH32V30xWxUx"
			(at 5.08 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at 0 5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.wch-ic.com/products/CH32V307.html?"
			(at 0 -5.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "The CH32V303/5/7 is an connectivity MCUs based on 32-bit RISC-V core."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RISC-V WCH MCU"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "QFN*8x8mm*P0.4mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32V30xWxUx_0_0"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32V30xWxUx_1_0"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "~{RST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN0" bidirectional line)
				(alternate "ETH_MII_CRS_WKUP" bidirectional line)
				(alternate "ETH_RGMII_RXD2" bidirectional line)
				(alternate "OPA4_OUT0" bidirectional line)
				(alternate "TIM2_CH1_ETR" bidirectional line)
				(alternate "TIM2_CH1_ETR_2" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "TIM8_ETR_1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "WKUP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN1" bidirectional line)
				(alternate "ETH_MII_RX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD3" bidirectional line)
				(alternate "ETH_RMII_REF_CLK" bidirectional line)
				(alternate "OPA3_OUT0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM9_BKIN_1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN2" bidirectional line)
				(alternate "ETH_MII_MDIO" bidirectional line)
				(alternate "ETH_RGMII_GXTC" bidirectional line)
				(alternate "ETH_RMII_MDIO" bidirectional line)
				(alternate "OPA2_OUT0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_CH3_1" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIM9_CH1_ETR_1" bidirectional line)
				(alternate "TIM9_ETR" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN3" bidirectional line)
				(alternate "ETH_MII_COL" bidirectional line)
				(alternate "ETH_RGMII_TXEN" bidirectional line)
				(alternate "OPA1_OUT0" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM2_CH4_1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIM9_CH2_1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN4" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM9_CH3" bidirectional line)
				(alternate "TIM9_CH3_1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN5" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "OPA2_CH1N" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM10_CH1N_1" bidirectional line)
				(alternate "USART1_CK_3" bidirectional line)
				(alternate "USART1_CTS_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN6" bidirectional line)
				(alternate "OPA1_CH1N" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH2N_1" bidirectional line)
				(alternate "TIM1_BKIN_1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART1_TX_3" bidirectional line)
				(alternate "USART7_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN7" bidirectional line)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RGMII_TXD0" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "OPA2_CH1P" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM10_CH3N_1" bidirectional line)
				(alternate "TIM1_CH1N_1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART1_RX_3" bidirectional line)
				(alternate "USART7_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "MCO" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH1_1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART1_CK_1" bidirectional line)
				(alternate "USART1_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OTG_FS_ID" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM1_CH3_1" bidirectional line)
				(alternate "USART1_CK_2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "OTG_FS_DM" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM1_CH4_1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "OTG_FS_DP" bidirectional line)
				(alternate "TIM10_CH1N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM1_ETR_1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1_ETR_1" bidirectional line)
				(alternate "TIM2_CH1_ETR_3" bidirectional line)
				(alternate "TIM8_CH3N_1" bidirectional line)
				(alternate "UART8_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN8" bidirectional line)
				(alternate "ETH_MII_RXD2" bidirectional line)
				(alternate "ETH_RGMII_TXD3" bidirectional line)
				(alternate "OPA1_CH1P" bidirectional line)
				(alternate "TIM1_CH2N_1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM3_CH3_2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TIM9_CH1N_1" bidirectional line)
				(alternate "UART4_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN9" bidirectional line)
				(alternate "ETH_MII_RXD3" bidirectional line)
				(alternate "ETH_RGMII_125IN" bidirectional line)
				(alternate "OPA4_CH0N" bidirectional line)
				(alternate "TIM1_CH3N_1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM3_CH4_2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "TIM9_CH2N_1" bidirectional line)
				(alternate "UART4_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "BOOT1" bidirectional line)
				(alternate "OPA3_CH0N" bidirectional line)
				(alternate "TIM9_CH3N_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_CH1_1" bidirectional line)
				(alternate "TIM2_CH2_1" bidirectional line)
				(alternate "TIM2_CH2_3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH2_1" bidirectional line)
				(alternate "TIM3_CH1_2" bidirectional line)
				(alternate "UART5_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_PPS_OUT" bidirectional line)
				(alternate "ETH_RMII_PPS_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_CH3_1" bidirectional line)
				(alternate "TIM3_CH2_2" bidirectional line)
				(alternate "UART5_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_CH1_1" bidirectional line)
				(alternate "USART1_TX_1" bidirectional line)
				(alternate "USBFS_DM" bidirectional line)
				(alternate "USBHS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_CH2_1" bidirectional line)
				(alternate "USART1_RX_1" bidirectional line)
				(alternate "USBFS_DP" bidirectional line)
				(alternate "USBHS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_RX" bidirectional line)
				(alternate "ETH_MII_TXD3" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIM8_CH3_1" bidirectional line)
				(alternate "UART6_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM10_CH2" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIM8_BKIN_1" bidirectional line)
				(alternate "UART6_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "OPA2_CH0N" bidirectional line)
				(alternate "TIM10_BKIN_1" bidirectional line)
				(alternate "TIM2_CH3_2" bidirectional line)
				(alternate "TIM2_CH3_3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_TX_EN" bidirectional line)
				(alternate "ETH_RMII_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "OPA1_CH0N" bidirectional line)
				(alternate "TIM10_ETR_1" bidirectional line)
				(alternate "TIM2_CH4_2" bidirectional line)
				(alternate "TIM2_CH4_3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_RX" bidirectional line)
				(alternate "ETH_MII_TXD0" bidirectional line)
				(alternate "ETH_RMII_TXD0" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OPA4_CH0P" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CAN2_TX" bidirectional line)
				(alternate "ETH_MII_TXD1" bidirectional line)
				(alternate "ETH_RMII_TXD1" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "OPA3_CH0P" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_CTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OPA2_CH0P" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART3_RTS_1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "OPA1_CH0P" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "USART1_TX_2" bidirectional line)
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "OSC_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD0" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "OSC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PD1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "SWDIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA13" bidirectional line)
				(alternate "TIM10_CH2N" bidirectional line)
				(alternate "TIM8_CH1N_1" bidirectional line)
				(alternate "USART3_TX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SWCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PA14" bidirectional line)
				(alternate "TIM10_CH3N" bidirectional line)
				(alternate "TIM8_CH2N_1" bidirectional line)
				(alternate "UART8_TX_1" bidirectional line)
				(alternate "USART3_RX_2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN10" bidirectional line)
				(alternate "ETH_RGMII_RXC" bidirectional line)
				(alternate "TIM9_CH1N" bidirectional line)
				(alternate "UART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN11" bidirectional line)
				(alternate "ETH_MII_MDC" bidirectional line)
				(alternate "ETH_RGMII_RXCTL" bidirectional line)
				(alternate "ETH_RMII_MDC" bidirectional line)
				(alternate "TIM9_CH2N" bidirectional line)
				(alternate "UART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN12" bidirectional line)
				(alternate "ETH_MII_TXD2" bidirectional line)
				(alternate "ETH_RGMII_RXD0" bidirectional line)
				(alternate "OPA3_CH1N" bidirectional line)
				(alternate "TIM9_CH3N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN13" bidirectional line)
				(alternate "ETH_MII_TX_CLK" bidirectional line)
				(alternate "ETH_RGMII_RXD1" bidirectional line)
				(alternate "OPA4_CH1N" bidirectional line)
				(alternate "TIM10_CH3" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN14" bidirectional line)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RGMII_TXD1" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "OPA4_CH1P" bidirectional line)
				(alternate "TIM9_CH4" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART1_CTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC_IN15" bidirectional line)
				(alternate "ETH_MII_RXD1" bidirectional line)
				(alternate "ETH_RGMII_TXD2" bidirectional line)
				(alternate "ETH_RMII_RDX1" bidirectional line)
				(alternate "OPA3_CH1P" bidirectional line)
				(alternate "TIM9_BKIN" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
				(alternate "USART1_RTS_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXP" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1_3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RXN" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2_3" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXP" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3_3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXN" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4_3" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM10_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM10_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM10_BKIN" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TAMPER-RTC" bidirectional line)
				(alternate "TIM8_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_IN" bidirectional line)
				(alternate "TIM9_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "OSC32_OUT" bidirectional line)
				(alternate "TIM10_CH4_1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIM3_ETR_2" bidirectional line)
				(alternate "TIM3_ETR_3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RX_DV" bidirectional line)
				(alternate "ETH_RMII_CRS_DV" bidirectional line)
				(alternate "TIM9_CH1N_2" bidirectional line)
				(alternate "USART3_TX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_MII_RXD0" bidirectional line)
				(alternate "ETH_RMII_RXD0" bidirectional line)
				(alternate "TIM9_CH1_ETR_2" bidirectional line)
				(alternate "USART3_RX_3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PE0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIM4_ETR_1" bidirectional line)
			)
		)
		(symbol "CH32V30xWxUx_1_1"
			(rectangle
				(start -12.7 48.26)
				(end 12.7 -48.26)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH32X035G8U6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 29.718 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH32X035G8U6"
			(at 8.636 29.718 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-28-1EP_4x4mm_P0.4mm_EP2.7x2.7mm"
			(at -0.254 3.556 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH32X035DS0_PDF.html"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "48MHz RISC-V MCU with USB PD phy (Sink, Source, DRP), USB 2.0 Full speed phy (Host, Device), 20KB RAM, 62KB Flash, WQFN-28"
			(at 1.016 3.556 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "microcontroller WCH Type-C"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.4mm*EP2.7x2.7*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH32X035G8U6_0_0"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PC3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PC10/PC17/UDP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PC11/PC16/UDM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC14/CC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC15/CC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC18/DIO"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC19/DCK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32X035G8U6_1_0"
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1/PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "CH32X035G8U6_1_1"
			(rectangle
				(start -12.7 27.94)
				(end 12.7 -27.94)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH592F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 26.67 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "CH592F"
			(at 6.35 26.67 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-28-1EP_4x4mm_P0.4mm_EP2.7x2.7mm"
			(at 0 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH592DS1_PDF.html"
			(at 0 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RISC-V core Bluetooth LE 5.4 MCU, USB 2.0 host / device, segment LCD driver, SPI, I2C / SMBus, 4 UART, 12-bit ADC, touch-key detection module, WQFN-28"
			(at 0 2.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "WCH WinChipHead microcontroller Bluetooth-Low-Energy BLE"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "*QFN*4x4mm?P0.4mm?EP2.7*x2.7*mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "CH592F_0_1"
			(rectangle
				(start -10.16 25.4)
				(end 10.16 -22.86)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "CH592F_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN0" input line)
				(alternate "RXD3" input line)
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN1" input line)
				(alternate "TXD3" output line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN12" input line)
				(alternate "RXD1" input line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN13" input line)
				(alternate "TMR0" bidirectional line)
				(alternate "TXD1" output line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TMR1" bidirectional line)
				(alternate "X32KI" input line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TMR2" bidirectional line)
				(alternate "~{X32KO}" output line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN2" input line)
				(alternate "PWM4" output line)
				(alternate "~{SCS}" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PA13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN3" input line)
				(alternate "PWM5" output line)
				(alternate "SCK0" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PA14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN4" input line)
				(alternate "MOSI" bidirectional line)
				(alternate "TXD0_" output line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "AIN5" input line)
				(alternate "MISO" bidirectional line)
				(alternate "RXD0_" input line)
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VSW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VDCID"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VDCIA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "VINTA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD33/VIO33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VBAT" power_in line)
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PWM7" output line)
				(alternate "RXD0" input line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PWM9" output line)
				(alternate "TXD0" output line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TMR1_" bidirectional line)
				(alternate "UD-" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "TMR2_" bidirectional line)
				(alternate "UD+" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "RI_" input line)
				(alternate "RXD1_" input line)
				(alternate "~{SCS_}" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCD_" input line)
				(alternate "SCK0_" bidirectional line)
				(alternate "TXD1_" output line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DSR" input line)
				(alternate "MOSI_" bidirectional line)
				(alternate "PWM10" output line)
				(alternate "SDA" bidirectional line)
				(alternate "TIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DTR" output line)
				(alternate "MISO_" bidirectional line)
				(alternate "SCL" bidirectional line)
				(alternate "TCK" input line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PB22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "RXD2" input line)
				(alternate "TMR3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PB23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PWM11" output line)
				(alternate "TMR0_" bidirectional line)
				(alternate "TXD2" output line)
				(alternate "~{RST}" input line)
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "X32MI"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{X32MO}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "ANT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
