(footprint "SIQ-02FVS3_Rotary_Encoder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -18.59 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "cfac5216-f2a4-43b8-a8a3-8d9a20dbd8c5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "RotaryEncoder_Switch"
		(at 0.095 22.315 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b7039ab8-5800-4368-98e4-06a675ce2553")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "30e10588-4d05-46b2-8225-3d843de76570")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1eb78be7-a003-4fe9-b64b-d6e15d715926")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.15 0)
		(end -5.15 7.25)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5454b3f3-f1a6-4416-967f-7557a8c0edd7")
	)
	(fp_line
		(start -5.15 7.25)
		(end 5.15 7.25)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6d8d172a-baca-44b4-ba07-8b87c3642da0")
	)
	(fp_line
		(start -4.199999 0)
		(end -5.15 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b844e832-e20b-4de1-8c80-650c74886087")
	)
	(fp_line
		(start 0 -3.842113)
		(end -1.696517 -3.842113)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e6e4fc68-8529-44b5-b5d7-510dc73d33c7")
	)
	(fp_line
		(start 0 -3.842113)
		(end 1.696517 -3.842113)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c63edd61-0dca-4845-98c9-63e808f15647")
	)
	(fp_line
		(start 5.15 0)
		(end 4.199999 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b885039b-4176-478a-aed1-1e7625532ddb")
	)
	(fp_line
		(start 5.15 7.25)
		(end 5.15 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0692eab2-338d-4fe4-b885-d3a0ea314c4f")
	)
	(fp_arc
		(start -4.199999 0)
		(mid -3.518903 -2.292883)
		(end -1.696517 -3.842113)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "177ac13b-eca9-4468-a977-a147ffb594e1")
	)
	(fp_arc
		(start 1.696517 -3.842113)
		(mid 3.518905 -2.292884)
		(end 4.199999 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b96c0c5e-1f86-4768-a67e-fdb4b5d5e7bf")
	)
	(fp_circle
		(center 0 0)
		(end 0.2 -7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "675227b2-2372-40c7-8800-554a44eea6b3")
	)
	(fp_poly
		(pts
			(xy -5.4 7.5) (xy 5.4 7.5) (xy 5.4 -0.2) (xy 4.4 -0.2) (xy 4.1 -1.6) (xy 3.3 -2.9) (xy 1.7 -4.1)
			(xy -1.7 -4.1) (xy -3.4 -2.9) (xy -4.1 -1.6) (xy -4.4 -0.2) (xy -5.4 -0.2)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "44ec1d26-449f-461b-b157-7b2b75285143")
	)
	(fp_circle
		(center 0 0)
		(end 7.25 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "User.6")
		(uuid "186b4c91-0796-4156-ba0e-9be167b5f492")
	)
	(fp_text user "${REFERENCE}"
		(at 2.000001 -2.5 270)
		(layer "F.Fab")
		(uuid "9a4c3400-30b6-451b-aba5-84c2377fcbe0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -3 4.5)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(uuid "b26a56b1-e995-40af-92a3-a4473e1d28c6")
	)
	(pad "" np_thru_hole circle
		(at 3 4.5)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(uuid "061fbad0-d8b4-405b-ae76-28174419ff6c")
	)
	(pad "0" smd roundrect
		(at -5.4 1.3 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "827e82ed-5646-492d-ad4d-68075f8653b6")
	)
	(pad "0" smd roundrect
		(at -5.4 5.4 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "a0d156a7-5823-4553-b259-8f8c6f3ed3ed")
	)
	(pad "0" smd roundrect
		(at -3.25269 -3.1 225)
		(size 0.85 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "583fe6a7-f78b-43fc-a5b0-55f2b7ec1f39")
	)
	(pad "0" smd roundrect
		(at 3.25266 -3.100001 315)
		(size 0.85 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "18c5843e-db55-4277-ae55-ac81d8fd562b")
	)
	(pad "0" smd roundrect
		(at 5.4 1.3 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "e4272445-67e0-4667-bd72-10bf442c3caf")
	)
	(pad "0" smd roundrect
		(at 5.4 5.4 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "62a8873b-99c7-4c16-9814-9dd3380862ee")
	)
	(pad "1" smd roundrect
		(at -4 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "1a1c002d-6430-4235-b381-b44f85ccadaa")
	)
	(pad "2" smd roundrect
		(at -1.475 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "fe6c6d32-71af-4331-90c6-3c1b706a68ac")
	)
	(pad "3" smd roundrect
		(at 1.475 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "aa1f4abd-3320-451d-97ac-c02d1d90a88c")
	)
	(pad "4" smd roundrect
		(at 4 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "2c66048c-2e15-407d-9227-36df952b177c")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/footprints/Custom.pretty/SIQ-02FVS3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
