
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32-S3-WROOM-1U-N8R8" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 31.242 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "ESP32-S3-WROOM-1U-N8R8" (id 1) (at -10.16 -33.02 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "ESP32-S3-WROOM-1U-N8R8:XCVR_ESP32-S3-WROOM-1U-N8R8" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Espressif Systems" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.35mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "SMD-41 Espressif Systems" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1U-N8R8/Espressif+Systems/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "v1.1" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32-S3-WROOM-1U-N8R8/Espressif+Systems/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "ESP32-S3-WROOM-1U-N8R8" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Bluetooth, WiFi 802.11b/g/n, Bluetooth v5.0 Transceiver Module 2.4GHz Antenna Not Included, U.FL Surface Mount\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Espressif Systems" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "ESP32-S3-WROOM-1U-N8R8_0_0"
      (rectangle (start -10.16 -30.48) (end 10.16 30.48)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "40"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -27.94 180.0) (length 5.08) hide
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "41_9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 27.94 180.0) (length 5.08)
        (name "3V3"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -15.24 25.4 0) (length 5.08)
        (name "EN"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 5.08 180.0) (length 5.08)
        (name "IO35"
          (effects (font (size 1.016 1.016)))
        )
        (number "28"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -22.86 180.0) (length 5.08)
        (name "IO48"
          (effects (font (size 1.016 1.016)))
        )
        (number "25"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -10.16 180.0) (length 5.08)
        (name "IO41"
          (effects (font (size 1.016 1.016)))
        )
        (number "34"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -5.08 180.0) (length 5.08)
        (name "IO39"
          (effects (font (size 1.016 1.016)))
        )
        (number "32"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -20.32 180.0) (length 5.08)
        (name "IO47"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -7.62 180.0) (length 5.08)
        (name "IO40"
          (effects (font (size 1.016 1.016)))
        )
        (number "33"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -22.86 0) (length 5.08)
        (name "IO14"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -17.78 0) (length 5.08)
        (name "IO12"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -20.32 0) (length 5.08)
        (name "IO13"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 22.86 180.0) (length 5.08)
        (name "IO15"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 5.08)
        (name "IO2"
          (effects (font (size 1.016 1.016)))
        )
        (number "38"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 5.08)
        (name "IO0"
          (effects (font (size 1.016 1.016)))
        )
        (number "27"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 5.08)
        (name "IO4"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 20.32 180.0) (length 5.08)
        (name "IO16"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 17.78 180.0) (length 5.08)
        (name "IO17"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 0.0 0) (length 5.08)
        (name "IO5"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 15.24 180.0) (length 5.08)
        (name "IO18"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 12.7 180.0) (length 5.08)
        (name "IO19"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 7.62 180.0) (length 5.08)
        (name "IO21"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 0.0 180.0) (length 5.08)
        (name "IO37"
          (effects (font (size 1.016 1.016)))
        )
        (number "30"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -2.54 180.0) (length 5.08)
        (name "IO38"
          (effects (font (size 1.016 1.016)))
        )
        (number "31"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 5.08)
        (name "IO1"
          (effects (font (size 1.016 1.016)))
        )
        (number "39"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 5.08)
        (name "IO3"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
        (name "IO6"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 5.08)
        (name "IO7"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 5.08)
        (name "IO8"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -10.16 0) (length 5.08)
        (name "IO9"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 5.08)
        (name "IO10"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 5.08)
        (name "IO11"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 2.54 180.0) (length 5.08)
        (name "IO36"
          (effects (font (size 1.016 1.016)))
        )
        (number "29"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -12.7 180.0) (length 5.08)
        (name "IO42"
          (effects (font (size 1.016 1.016)))
        )
        (number "35"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 10.16 180.0) (length 5.08)
        (name "IO20"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 5.08)
        (name "TXD0"
          (effects (font (size 1.016 1.016)))
        )
        (number "37"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 5.08)
        (name "RXD0"
          (effects (font (size 1.016 1.016)))
        )
        (number "36"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -15.24 180.0) (length 5.08)
        (name "IO45"
          (effects (font (size 1.016 1.016)))
        )
        (number "26"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -17.78 180.0) (length 5.08)
        (name "IO46"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)