(footprint "C4B1802110"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Push Button")
	(tags "Button Push SMD")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "32e5de83-9409-498a-b4bb-3938c97d4948")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "C4B1802110"
		(at 0 2.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3f54b9c2-4298-492d-bb06-ef54a3764527")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.lcsc.com/datasheet/C49393608.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9b6eb576-70c4-45ea-a760-8b6264c09910")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "SMD Push Button 3mmx4,6mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1277b4a-d64d-4abd-ad83-aa948f8dff69")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.2 0.05)
		(end -2.2 -0.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0dc52c37-e52f-4f4c-b287-92e6cffafaec")
	)
	(fp_line
		(start -2.2 1.55)
		(end 2.2 1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7f6229cc-189e-42bb-ac88-0145f9159303")
	)
	(fp_line
		(start 2.2 -1.55)
		(end -2.2 -1.55)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c3327a33-fe33-4923-a5b8-6a10cd576c11")
	)
	(fp_line
		(start 2.2 0.05)
		(end 2.2 -0.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "64380adc-a690-4e48-be4e-fa0e2960e779")
	)
	(fp_line
		(start -3.25 -1.8)
		(end 3.25 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e0bab0d8-797a-413a-8657-7ce3be67492e")
	)
	(fp_line
		(start -3.25 1.8)
		(end -3.25 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6652325d-a232-41ec-806f-8102d50e3053")
	)
	(fp_line
		(start 3.25 -1.8)
		(end 3.25 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4140022d-6731-4b08-a6ea-40983dc1e1bd")
	)
	(fp_line
		(start 3.25 1.8)
		(end -3.25 1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "89cbf054-b4e0-434e-816f-24dbacca4544")
	)
	(fp_line
		(start -2.1 -1.4)
		(end 2.1 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a4ad80ff-9e0d-4c85-af54-b56a34037f8f")
	)
	(fp_line
		(start -2.1 1.4)
		(end -2.1 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fda18a33-6f63-4227-9bea-b92e9c664b5f")
	)
	(fp_line
		(start 2.1 -1.4)
		(end 2.1 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cba54ea1-41d1-4112-8483-85ee70691510")
	)
	(fp_line
		(start 2.1 1.4)
		(end -2.1 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "27aca447-38ec-427f-8c09-01898eac2224")
	)
	(fp_circle
		(center 0 0)
		(end 0 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "9129029f-bd94-432f-b09a-f2188dc79ec0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 4.4 0)
		(layer "F.Fab")
		(uuid "ed1e34c1-b963-441e-bb76-35b70031f53d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.3 -0.8)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e02251f0-7c48-4224-954a-296af71ed054")
	)
	(pad "1" smd rect
		(at 2.3 -0.8)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5711d49d-d5dc-4ad8-9c76-7895d30de493")
	)
	(pad "2" smd rect
		(at -2.3 0.8)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "3fbaa6b0-08ce-42bd-b412-35f884a50bdc")
	)
	(pad "2" smd rect
		(at 2.3 0.8)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "801b888b-f475-4c15-984c-433318578c3f")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/footprints/Buttons.pretty/C4B1802110.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
