
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "LSM6DSO32TR" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 16.002 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "LSM6DSO32TR" (id 1) (at -12.7 -17.78 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "LSM6DSO32TR:XDCR_LSM6DSO32TR" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "DigiKey_Part_Number" "497-LSM6DSO32CT-ND" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/LSM6DSO32TR/STMicroelectronics/view-part/?ref=snap" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.86mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "VFLGA-14 STMicroelectronics" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/LSM6DSO32TR/STMicroelectronics/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "1" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "STMicroelectronics" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "LSM6DSO32TR" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Accelerometer, Gyroscope, Temperature, 6 Axis Sensor I2C, SPI Output\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "STMicroelectronics" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "LSM6DSO32TR_0_0"
      (rectangle (start -12.7 -15.24) (end 12.7 15.24)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at 17.78 -5.08 180.0) (length 5.08)
        (name "SDO/SA0"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -2.54 0) (length 5.08)
        (name "SDX"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 0.0 0) (length 5.08)
        (name "SCX"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -17.78 5.08 0) (length 5.08)
        (name "INT1"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 10.16 180.0) (length 5.08)
        (name "VDDIO"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -12.7 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -12.7 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 12.7 180.0) (length 5.08)
        (name "VDD"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 17.78 5.08 180.0) (length 5.08)
        (name "INT2"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at -17.78 -7.62 0) (length 5.08)
        (name "NC"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at -17.78 -7.62 0) (length 5.08)
        (name "NC"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at 17.78 -7.62 180.0) (length 5.08)
        (name "CS"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at 17.78 0.0 180.0) (length 5.08)
        (name "SCL"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "SDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)